FileInfo;;;;9d23;1;5;0;4;; ; ; ; ; ;152
Symbol name;;;;Name;Add;Size (bytes);Bits;Min Value;Max Value;Type;Common User;Site Responsible;Service Technician;Help text;Key
user_data.demo_1_beep;;;;Demo.Message 1.Beep;393;1;;0;7;Integer;;;R/W;Beep code used with demo message 1.;622
user_data.demo_1_text;;;;Demo.Message 1.Text;343;50;;;;Text;;;R/W;Display message shown for demo message 1, max 50 characters.;647
user_data.demo_2_beep;;;;Demo.Message 2.Beep;414;1;;0;7;Integer;;;R/W;Beep code used with demo message 2.;643
user_data.demo_2_text;;;;Demo.Message 2.Text;394;20;;;;Text;;;R/W;Display message shown for demo message 2, max 20 characters.;668
user_data.hot_key;;;;Hot key.Key;416;25;;;;REC10;R/W;R/W;R/W;Hot key;807
user_data.hot_key.index;;;;Hot key.Key.Function;416;1;;0;8;Integer;R/W;R/W;R/W;This is an index to a function (0-8);819
user_data.hot_key.functionality;;;;Hot key.Key.Functionality;417;1;;0;2;Integer;R/W;R/W;R/W;Defines if the hot key is linked to a function or a phone number. 0=Unused, 1 = Function , 2 = Telephone Number;897
user_data.hot_key.hot_data;;;;Hot key.Key.Telephone Number;418;23;;;;Text;R/W;R/W;R/W;Telephone number used with this hot-key.;850
subscr_dbase.ipei;;;;IPDI;215;5;;;;IPEI;R;R;R;IPDI;567
user_data.lock_code;;;;Lock code.Code;251;4;;;;Text; ;R/W;R/W;Code to be used when locking and unlocking phone.;614
user_data.ee_uif_flag.phone_locked;;;;Lock code.Phone locked;236;;7;0;1;Boolean; ;R/W;R/W;Phone lock ON/OFF;565
user_data.ee_ind_flag.ALS_ind;;;;Movement detector.ALS indication enabled;250;;2;0;1;Boolean; ;R/W;R/W;Alarm location signal ON/OFF;585
user_data.md_timer.duration_als;;;;Movement detector.ALS indication time;249;1;;;;Integer; ;R/W;R/W;Alarm location signal indication time;601
user_data.md_timer.duration_mdw.f.duration_mdw;;;;Movement detector.Duration;248;;0-6;0;127;Integer; ;R/W;R/W;Man down warning time in seconds;739
user_data.ee_uif_flag.MD_enable;;;;Movement detector.Enable movement detector;236;;6;0;1;Boolean;R/W;R/W;R/W;Movement detector ON/OFF;621
user_data.md_timer.duration_mdw.f.long_delay;;;;Movement detector.Extra delay;248;;7;0;1;Boolean; ;R/W;R/W;Enables 10 minutes extra delay before next man down detection.;632
user_data.md_timer.time_before_mdw.f.time_before_mdw;;;;Movement detector.Time before warning;247;;0-6;0;127;Integer; ;R/W;R/W;Specifies time before man down warning is started.;762
user_data.md_timer.time_before_mdw.f.resolution;;;;Movement detector.Time before warning in minutes;247;;7;0;1;Boolean; ;R/W;R/W;If this parameter is enabled 'Time before warning' is specified in minutes otherwise it is specified in seconds.;684
Phone_book;;;;Phone book.Index;1096;40;;;;REC75;R/W;R/W;R/W;;1488
Phone_book.Name;;;;Phone book.Index.Name;1096;17;;;;Text;R/W;R/W;R/W;Name to be shown.;1488
Phone_book.Number;;;;Phone book.Index.Number;1113;23;;;;Text;R/W;R/W;R/W;Number to dial;1510
user_data.ptt_dtmf_tone_push;;;;PTT.DTMF tone on push;341;1;;;;Hex;;;R/W;DTMF tone to send when mute key is pushed.;572
user_data.ptt_dtmf_tone_release;;;;PTT.DTMF tone on release;342;1;;;;Hex;;;R/W;DTMF tone to send when mute key is released.;578
user_data.ee_uif_flag.mute_key_as_ptt_enable;;;;PTT.Enable PTT on mute key;235;;3;0;1;Boolean;;;R/W;If mute key is to be used as PTT button when on conversation or not. When PTT button enabled it is not possible to mute in conversation.;575
eesubscr_record;;;;Registrations.System;42;43;;;;REC4;;;R;;269
eesubscr_record.flags.b.GAP_is;;;;Registrations.System.Flags.GAP_is;42;;1;0;1;Boolean;;;R;;230
eesubscr_record.flags.b.ipui_is;;;;Registrations.System.Flags.ipui_is;43;;1;0;1;Boolean;;;R;;232
eesubscr_record.flags.b.ipui_length_is;;;;Registrations.System.Flags.ipui_length_is;43;;0;0;1;Boolean;;;R;;239
eesubscr_record.flags.b.lal_is;;;;Registrations.System.Flags.lal_is;43;;6;0;1;Boolean;;;R;;231
eesubscr_record.flags.b.park_is;;;;Registrations.System.Flags.park_is;43;;2;0;1;Boolean;;;R;;232
eesubscr_record.flags.b.pli_is;;;;Registrations.System.Flags.pli_is;43;;3;0;1;Boolean;;;R;;231
eesubscr_record.flags.b.service_class_is;;;;Registrations.System.Flags.service_class_is;43;;7;0;1;Boolean;;;R;;241
eesubscr_record.flags.b.uak_ac_indicator;;;;Registrations.System.Flags.uak_ac_indicator;42;;0;0;1;Boolean;;;R;;240
eesubscr_record.flags.b.uak_ac_is;;;;Registrations.System.Flags.uak_ac_is;43;;4;0;1;Boolean;;;R;;234
eesubscr_record.flags.b.zap_field_is;;;;Registrations.System.Flags.zap_field_is;43;;5;0;1;Boolean;;;R;;237
eesubscr_record.ipui;;;;Registrations.System.IPUI;51;13;;;;Hex;;;R;IPUI;246
eesubscr_record.ipui_length;;;;Registrations.System.IPUI length;44;1;;;;Hex;;;R;Length of IPUI;244
eesubscr_record.lal;;;;Registrations.System.LAL;47;1;;;;Hex;;;R;Location Area Level;244
eesubscr_record.park;;;;Registrations.System.PARK;64;5;;;;Hex;;;R;PARK;251
eesubscr_record.pli;;;;Registrations.System.PLI;45;1;;;;Hex;;;R;Park Length Indicator;244
eesubscr_record.service_class;;;;Registrations.System.Service Class;48;1;;;;Hex;;;R;Service Class;249
eesubscr_record.uak_ac;;;;Registrations.System.UAK_AC;69;16;;;;Hex;;;R;UAK / AC;273
eesubscr_record.zap_field;;;;Registrations.System.ZAP field;46;1;;;;Hex;;;R;ZAP field;239
user_data.ee_uif_flag.auto_key_lock_enable;;;;Settings.Automatic key lock;235;;4;0;1;Boolean;R/W;R/W;R/W;Enables key lock to automatic turn on when idledisplay shown for 20 seconds;682
user_data.shared_line_indication_time;;;;Settings.CLIP indication time;415;1;;;;Integer;;;R/W;How many seconds a CLIP is shown when using shared lines.;675
user_data.ee_language_code;;;;Settings.Language;229;1;;0;9;Integer;R/W;R/W;R/W;Selects which language used in menus.;637
user_data.ee_ind_flag.Ongoing_conv_ind;;;;Settings.Off hook indication;250;;1;0;1;Boolean; ;R/W;R/W;Off hook indication ON/OFF;592
user_data.ee_uif_flag.overload_text_enable;;;;Settings.Overload text enabled;235;;2;0;1;Boolean; ; ;R/W;Overload text ON/OFF;523
user_data.ee_uif_flag.Direct_Offhook;;;;Settings.Quick answer;236;;5;0;1;Boolean;R/W;R/W;R/W;Quick answer ON/OFF;621
user_data.ee_ind_flag.Repeat_mess_ind;;;;Settings.Repeate message indication;250;;0;0;1;Boolean; ;R/W;R/W;When enabled message indication is repeated in 60 s.;617
user_data.ee_uif_flag.send_in_charger_status;;;;Settings.Send in charger status;235;;5;0;1;Boolean;;R/W;R/W;Enables transmission of charger status when handset placed into / removed from charger;610
user_data.ee_uif_flag.enable_test_functions;;;;Settings.Test function enabled;235;;1;0;1;Boolean;;R/W;R/W;Test function ON/OFF. When test functions enabled hot-keys are disabled.;595
user_data.ee_GeneralUserConfig.b.sys_busybeep_enable;;;;Settings.Tones.Busy beep;244;;0;0;1;Boolean; ; ;R/W;Enables beep when system busy.;552
user_data.ee_uif_flag.Ear_loud;;;;Settings.Tones.Ear volume;236;;0-1;0;3;Integer;R/W;R/W;R/W;Ear volume used when in conversation.;644
user_data.ee_uif_flag.Keyclick;;;;Settings.Tones.Keyclick;236;;2;0;1;Boolean;R/W;R/W;R/W;Key beep ON/OFF;611
user_data.ee_uif_flag.Knocking;;;;Settings.Tones.Knocking;236;;4;0;1;Boolean; ;R/W;R/W;Knocking ON/OFF;559
user_data.ee_uif_flag.Range_warning;;;;Settings.Tones.Range warning;236;;3;0;1;Boolean; ;R/W;R/W;Range warning ON/OFF;569
user_data.ee_beeper_user_def.melody;;;;Settings.Tones.Ring Melody;231;1;;0;6;Integer;R/W;R/W;R/W;Ring melody used when indication an incomming call.;659
user_data.ee_beeper_user_def.cadence;;;;Settings.Tones.Ring Speed;232;;0-2;0;6;Integer;R/W;R/W;R/W;Ring speed used when indication an incomming call;661
user_data.ee_beeper_user_def.volume;;;;Settings.Tones.Ring Volume;232;;3-5;0;4;Integer;R/W;R/W;R/W;Volume used when indicating an incomming call or message.;666
user_data.ee_trembler_flag.Trembler_enable;;;;Settings.Trembler enabled;245;;0;0;1;Boolean;R/W;R/W;R/W;Trembler ON/OFF;632
sim_version;;;;Sim version;0;2;;;;Hex;R;R;R;Sim version for parameter version 01.05;376
user_data.system_a_text;;;;System text.System A;289;12;;;;Text;;R/W;R/W;Text to be shown for System A.;612
user_data.system_b_text;;;;System text.System B;302;12;;;;Text;;R/W;R/W;Text to be shown for System B.;625
user_data.system_c_text;;;;System text.System C;315;12;;;;Text;;R/W;R/W;Text to be shown for System C.;638
user_data.system_d_text;;;;System text.System D;328;12;;;;Text;;R/W;R/W;Text to be shown for System D.;651
user_data.userid_text;;;;User id;276;12;;;;Text;R/W;R/W;R/W;User id;659
user_data.ee_environment;;;;Variables.ee_environment;228;1;;;;Integer;;;R;Defines currently selected system (A-D).;456
user_data.ee_GAB;;;;Variables.ee_GAB;237;6;;;;Hex; ; ;R;;483
user_data.ee_uif_flag.key_beep_before_locked;;;;Variables.key_beep_before_locked;235;;0;0;1;Boolean; ; ;R;;503
subscr_dbase.old_ari_rpn;;;;Variables.old_ari_rpn;221;5;;;;Hex;;;R;;408
subscr_dbase.flags.b.old_ari_rpn_is;;;;Variables.old_ari_rpn_is;214;;1;0;1;Boolean;;;R;;407
subscr_dbase.old_lal;;;;Variables.old_lal;220;1;;;;Hex;;;R;;399
subscr_dbase.flags.b.old_lal_is;;;;Variables.old_lal_is;214;;0;0;1;Boolean;;;R;;403
user_data.ee_ringer_set;;;;Variables.ringer_set;230;1;;0;4;Integer; ;R/W;R/W;Defines which set of ringing melodies to be used.;590
sim_9d23_text;;;;Variables.sim_9d23_text;5;4;;;;Text;R;R;R;Type of Handset;374
sim_factory_data.sim_country;;;;Variables.sim_country;13;1;;;;Hex;;;R;;200
sim_factory_data.sim_customer;;;;Variables.sim_customer;14;1;;;;Hex;;;R;;202
sim_factory_data.sim_design_code;;;;Variables.sim_design_code;24;1;;;;Hex;;;R;;215
sim_device_id;;;;Variables.sim_device_id;3;1;;;;Hex;R;R;R;Sim Card ID: xy    x=0 Size=4K, x=1 Size=8K, x=2 size=16K, y=1 9d23, y=2 9d24, y=3 Office155;433
sim_factory_data.sim_fertigung_bc;;;;Variables.sim_fertigung_bc;21;3;;;;Hex;;;R/W;;217
sim_factory_data.sim_fertigung_et;;;;Variables.sim_fertigung_et;18;3;;;;Hex;;;R/W;;214
sim_factory_data.sim_fertigung_ft;;;;Variables.sim_fertigung_ft;15;3;;;;Hex;;;R/W;;211
sim_first_mark;;;;Variables.sim_first_mark;4;1;;;;Hex;;;;;94
sim_factory_data.sim_hardware_version;;;;Variables.sim_hardware_version;25;1;;;;Hex;;;R;;221
sim_spare_bytes;;;;Variables.sim_spare_bytes;26;16;;;;Hex;;;R/W;;217
