

Copyright (C) HP Corporation 1990-2010.
All rights reserved.
HP Array Controller Firmware Ver = 3.00, Build Num = 0
   BootBlock Ver = 2.07, HAL-PL Ver = 02.03.011.001
Compiled Feb 17 2010 14:42:36

PASSED: HAL API Initialization
FirstAvail : 0x80a1be40


Initializing Memory...

Physical Requests    1407
Logical Requests     1024
Command Lists        1025
Local Memory Avail      10735376 bytes in 5 fragments
Shared Memory Avail     8388600 bytes in 2 fragments
Logical Reqs Avail      1024
Physical Reqs Avail     1407
Host Prefetch is ENABLED
PASSED: Memory Initialization

SSID = 3245103c
PASSED: I2C Initialization

NVRAM Update: ILA returned 0x0
PASSED: Bootstrap NVRAM Checksum

Platform NVRAM auto-update found an embedded image, but it is not an upgrade

PASSED: Command I/O Initialization
PASSED: Timer Initialization

Board is Marble     Rev. C
Using WWID to generate new board serial #: 5001438007E874E
NumMgmtDevices = 105 MgmtDeviceStartIndex = 146
num_drive_params_entries = 255 drive params size = 49980

Diagnostic Pointers Initialized
Diagnostic download address = 0x817e8000
Initializing XOR Engine...
validate_pic_fw: pic version in ROM = 52
Battery 1 not present.
Battery 2 not present.
Battery 3 not present.

Battery Status:    Battery 1      Battery 2      Battery 3
---------------    ---------      ---------      ---------
Present:               NO             NO             NO
Responding:           N/A            N/A            N/A


Found 256 MB of cache memory.
wcxc_ram_start = 0x47000000
wcxc_ram_size  = 0x09000000
DIMM SN: PACCQ9SYWI29
Initializing ADG for SAS controllers only (tolerate 8 drive failure)
ADG keys initialized

Starting DMA SelfTest
   Pattern Fill DMA mem write xfer rate:         1673 MB/sec
   Pattern Fill DMA mem read xfer rate:          1874 MB/sec
   Zero Pattern Fill DMA mem write xfer rate:    1669 MB/sec
   Zero Pattern Fill DMA mem read xfer rate:     1872 MB/sec
   Mem-to-mem DMA xfer rate:                     909 MB/sec
   Mem-to-WXOR DMA xfer rate:                    624 MB/sec
   Mem-to-WXOR Multicast xfer rate:              793 MB/sec
   Mem-to-Mem DMA_SendCDB xfer rate:             156 MB/sec
   Mem-to-Mem DMA_SendCDB w/XOR xfer rate:       179 MB/sec
ADG SelfTestOK

PASSED: DMAXOR Controller Initialization

PASSED: Cache Controller Initialization

PAL_CO_Init: tbl_entries = 255 size = 142800
Start Up Complete
Memory start 47000000
Memory size 9000000
Cache Mem Test PASSED!


Pre-discovery LF: DIS: 0x00, SL_SAS: 0x00, SL_SATA: 0x00, LFV: 0x03, PBP: 0xff

Protocol device 0 scan devices started
Protocol device 0 scan devices done
Adapter 0 Bus Reset
PR 80aa10b8h:D000 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:02
PR 80aa10b8h:D001 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:02
PR 80aa10b8h:D002 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:02
PR 80aa10b8h:D250 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
get_drive_params: Inquiry to SEP for VPD page to get serial # failed.
Updated full box tbl in RIS

Configured logical unit (volume) count = 1
   ccf=0x00, mccf=0x00000000
Array A Unit 0: RAID 5; df=128 vs=OK drvs=3 dd=2 pg=1 vofs=0x000000000 blks=0x0222CE330 ca=ena srf=0x1 dt=2
  U0 drive map (hex) = 00 01 02
Controller WWID = 5001438007e874e0

*****  Discovered SAS (Compatible) Devices  ****
D000 p0|01 P1I[00-01]:Disk HP      DG0146FARVU     ,HPD8,WWID=5000cca0:0adf7b79, 10K
D001 p0|01 P1I[00-02]:Disk HP      DG0146FARVU     ,HPD8,WWID=5000cca0:0ae013c1, 10K
D002 p0|01 P1I[00-03]:Disk HP      DG0146FARVU     ,HPD8,WWID=5000cca0:0adc2171, 10K
D250 p0|01 ???[??-00]:SEP  PMCSIERA SRC 8x6G       ,RevC,WWID=50014380:07e874ef
D251 p0|01 ???[??-00]:SGPIO                        ,    ,WWID=50014380:07e874e0
D253                 :Protocol Adapter
D254                 :Protocol Adapter
Total Discovered SAS  Devices:  3

*****  Onboard PHY Link Rates  ****
   \PHYS         0          10         20         30         40
Onboard Phys   : AAA00000

*****  Expander PHY Link Rates  ****
EXP\PHYS         0          10         20         30         40
Total 6.0G Links:  3
DirtyQMemBytes: 147456
Local Memory Avail      7772092 bytes in 43 fragments
Shared Memory Avail     8367492 bytes in 17 fragments
Logical Reqs Avail      1023
Physical Reqs Avail     1020
Host Prefetch is ENABLED
ROM Flash Driver Init Passed
Testing ROM Image A
Testing ROM Image B
PCI rev. 0x1 using 4 lanes @5.0G

Host-to-local data xfer rate, using CPU:  638 MB/sec
Host-to-local data xfer rate, using DMA:  1398 MB/sec
Host time is 1:29:57, 4/19/2011
PCI slot 0
Periodic iLO command check interval=1 seconds, hostaddr=0x0DF63E020.
Host time is 1:29:59, 4/19/2011
PCI slot 0

[04/19 01:29:59]

Run-Time LF: DIS: 0x00, SL_SAS: 0x00, SL_SATA: 0x00, LFV: 0x03, PBP: 0xff

[04/19 01:30:02]Local-to-host data xfer rate, using DMA:  1459 MB/sec
[04/19 01:30:02]Int13 BIOS unit 0x80 = CISS LUN 0x4000000000000000 


Copyright (C) HP Corporation 1990-2010.
All rights reserved.
HP Array Controller Firmware Ver = 3.00, Build Num = 0
   BootBlock Ver = 2.07, HAL-PL Ver = 02.03.011.001
Compiled Feb 17 2010 14:42:36

PASSED: HAL API Initialization
FirstAvail : 0x80a1be40


Initializing Memory...

Physical Requests    1407
Logical Requests     1024
Command Lists        1025
Local Memory Avail      10735376 bytes in 5 fragments
Shared Memory Avail     8388600 bytes in 2 fragments
Logical Reqs Avail      1024
Physical Reqs Avail     1407
Host Prefetch is ENABLED
PASSED: Memory Initialization

SSID = 3245103c
PASSED: I2C Initialization

NVRAM Update: ILA returned 0x0
PASSED: Bootstrap NVRAM Checksum

Platform NVRAM auto-update found an embedded image, but it is not an upgrade

PASSED: Command I/O Initialization
PASSED: Timer Initialization

Board is Marble     Rev. C
Using WWID to generate new board serial #: 5001438007E874E
NumMgmtDevices = 105 MgmtDeviceStartIndex = 146
num_drive_params_entries = 255 drive params size = 49980

Diagnostic Pointers Initialized
Diagnostic download address = 0x817e8000
Initializing XOR Engine...
validate_pic_fw: pic version in ROM = 52
Battery 1 not present.
Battery 2 not present.
Battery 3 not present.

Battery Status:    Battery 1      Battery 2      Battery 3
---------------    ---------      ---------      ---------
Present:               NO             NO             NO
Responding:           N/A            N/A            N/A


Found 256 MB of cache memory.
wcxc_ram_start = 0x47000000
wcxc_ram_size  = 0x09000000
DIMM SN: PACCQ9SYWI29
Initializing ADG for SAS controllers only (tolerate 8 drive failure)
ADG keys initialized

Starting DMA SelfTest
   Pattern Fill DMA mem write xfer rate:         1673 MB/sec
   Pattern Fill DMA mem read xfer rate:          1873 MB/sec
   Zero Pattern Fill DMA mem write xfer rate:    1669 MB/sec
   Zero Pattern Fill DMA mem read xfer rate:     1872 MB/sec
   Mem-to-mem DMA xfer rate:                     896 MB/sec
   Mem-to-WXOR DMA xfer rate:                    611 MB/sec
   Mem-to-WXOR Multicast xfer rate:              780 MB/sec
   Mem-to-Mem DMA_SendCDB xfer rate:             168 MB/sec
   Mem-to-Mem DMA_SendCDB w/XOR xfer rate:       176 MB/sec
ADG SelfTestOK

PASSED: DMAXOR Controller Initialization

PASSED: Cache Controller Initialization

PAL_CO_Init: tbl_entries = 255 size = 142800
Start Up Complete
Memory start 47000000
Memory size 9000000
Cache Mem Test PASSED!


Pre-discovery LF: DIS: 0x00, SL_SAS: 0x00, SL_SATA: 0x00, LFV: 0x03, PBP: 0xff

Protocol device 0 scan devices started
Protocol device 0 scan devices done
Adapter 0 Bus Reset
PR 80aa10b8h:D000 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:02
PR 80aa10b8h:D001 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:02
PR 80aa10b8h:D002 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:02
PR 80aa10b8h:D250 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
get_drive_params: Inquiry to SEP for VPD page to get serial # failed.
Updated full box tbl in RIS

Configured logical unit (volume) count = 1
   ccf=0x00, mccf=0x00000000
Array A Unit 0: RAID 5; df=128 vs=OK drvs=3 dd=2 pg=1 vofs=0x000000000 blks=0x0222CE330 ca=ena srf=0x1 dt=2
  U0 drive map (hex) = 00 01 02
Controller WWID = 5001438007e874e0

*****  Discovered SAS (Compatible) Devices  ****
D000 p0|01 P1I[00-01]:Disk HP      DG0146FARVU     ,HPD8,WWID=5000cca0:0adf7b79, 10K
D001 p0|01 P1I[00-02]:Disk HP      DG0146FARVU     ,HPD8,WWID=5000cca0:0ae013c1, 10K
D002 p0|01 P1I[00-03]:Disk HP      DG0146FARVU     ,HPD8,WWID=5000cca0:0adc2171, 10K
D250 p0|01 ???[??-00]:SEP  PMCSIERA SRC 8x6G       ,RevC,WWID=50014380:07e874ef
D251 p0|01 ???[??-00]:SGPIO                        ,    ,WWID=50014380:07e874e0
D253                 :Protocol Adapter
D254                 :Protocol Adapter
Total Discovered SAS  Devices:  3

*****  Onboard PHY Link Rates  ****
   \PHYS         0          10         20         30         40
Onboard Phys   : AAA00000

*****  Expander PHY Link Rates  ****
EXP\PHYS         0          10         20         30         40
Total 6.0G Links:  3
DirtyQMemBytes: 147456
Local Memory Avail      7772092 bytes in 43 fragments
Shared Memory Avail     8367492 bytes in 17 fragments
Logical Reqs Avail      1023
Physical Reqs Avail     1024
Host Prefetch is ENABLED
ROM Flash Driver Init Passed
Testing ROM Image A
Testing ROM Image B
PCI rev. 0x1 using 4 lanes @5.0G

Host-to-local data xfer rate, using CPU:  662 MB/sec
Host-to-local data xfer rate, using DMA:  1395 MB/sec
Host time is 1:04:17, 4/24/2011
PCI slot 0
Periodic iLO command check interval=1 seconds, hostaddr=0x0DF63E020.
Host time is 1:04:19, 4/24/2011
PCI slot 0

[04/24 01:04:19]

Run-Time LF: DIS: 0x00, SL_SAS: 0x00, SL_SATA: 0x00, LFV: 0x03, PBP: 0xff

[04/24 01:04:22]Local-to-host data xfer rate, using DMA:  1452 MB/sec
[04/24 01:04:22]Int13 BIOS unit 0x80 = CISS LUN 0x4000000000000000 


Copyright (C) HP Corporation 1990-2010.
All rights reserved.
HP Array Controller Firmware Ver = 3.00, Build Num = 0
   BootBlock Ver = 2.07, HAL-PL Ver = 02.03.011.001
Compiled Feb 17 2010 14:42:36

PASSED: HAL API Initialization
FirstAvail : 0x80a1be40


Initializing Memory...

Physical Requests    1407
Logical Requests     1024
Command Lists        1025
Local Memory Avail      10735376 bytes in 5 fragments
Shared Memory Avail     8388600 bytes in 2 fragments
Logical Reqs Avail      1024
Physical Reqs Avail     1407
Host Prefetch is ENABLED
PASSED: Memory Initialization

SSID = 3245103c
PASSED: I2C Initialization

NVRAM Update: ILA returned 0x0
PASSED: Bootstrap NVRAM Checksum

Platform NVRAM auto-update found an embedded image, but it is not an upgrade

PASSED: Command I/O Initialization
PASSED: Timer Initialization

Board is Marble     Rev. C
Using WWID to generate new board serial #: 5001438007E874E
NumMgmtDevices = 105 MgmtDeviceStartIndex = 146
num_drive_params_entries = 255 drive params size = 49980

Diagnostic Pointers Initialized
Diagnostic download address = 0x817e8000
Initializing XOR Engine...
validate_pic_fw: pic version in ROM = 52
Battery 1 not present.
Battery 2 not present.
Battery 3 not present.

Battery Status:    Battery 1      Battery 2      Battery 3
---------------    ---------      ---------      ---------
Present:               NO             NO             NO
Responding:           N/A            N/A            N/A


Found 256 MB of cache memory.
wcxc_ram_start = 0x47000000
wcxc_ram_size  = 0x09000000
DIMM SN: PACCQ9SYWI29
Initializing ADG for SAS controllers only (tolerate 8 drive failure)
ADG keys initialized

Starting DMA SelfTest
   Pattern Fill DMA mem write xfer rate:         1671 MB/sec
   Pattern Fill DMA mem read xfer rate:          1872 MB/sec
   Zero Pattern Fill DMA mem write xfer rate:    1669 MB/sec
   Zero Pattern Fill DMA mem read xfer rate:     1872 MB/sec
   Mem-to-mem DMA xfer rate:                     907 MB/sec
   Mem-to-WXOR DMA xfer rate:                    622 MB/sec
   Mem-to-WXOR Multicast xfer rate:              795 MB/sec
   Mem-to-Mem DMA_SendCDB xfer rate:             164 MB/sec
   Mem-to-Mem DMA_SendCDB w/XOR xfer rate:       166 MB/sec
ADG SelfTestOK

PASSED: DMAXOR Controller Initialization

PASSED: Cache Controller Initialization

PAL_CO_Init: tbl_entries = 255 size = 142800
Start Up Complete
Memory start 47000000
Memory size 9000000
Cache Mem Test PASSED!


Pre-discovery LF: DIS: 0x00, SL_SAS: 0x00, SL_SATA: 0x00, LFV: 0x03, PBP: 0xff

Protocol device 0 scan devices started
Protocol device 0 scan devices done
Adapter 0 Bus Reset
PR 80aa10b8h:D000 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:02
PR 80aa10b8h:D001 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:02
PR 80aa10b8h:D002 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:02
PR 80aa10b8h:D250 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
get_drive_params: Inquiry to SEP for VPD page to get serial # failed.
Updated full box tbl in RIS

Configured logical unit (volume) count = 1
   ccf=0x00, mccf=0x00000000
Array A Unit 0: RAID 5; df=128 vs=OK drvs=3 dd=2 pg=1 vofs=0x000000000 blks=0x0222CE330 ca=ena srf=0x1 dt=2
  U0 drive map (hex) = 00 01 02
Controller WWID = 5001438007e874e0

*****  Discovered SAS (Compatible) Devices  ****
D000 p0|01 P1I[00-01]:Disk HP      DG0146FARVU     ,HPD8,WWID=5000cca0:0adf7b79, 10K
D001 p0|01 P1I[00-02]:Disk HP      DG0146FARVU     ,HPD8,WWID=5000cca0:0ae013c1, 10K
D002 p0|01 P1I[00-03]:Disk HP      DG0146FARVU     ,HPD8,WWID=5000cca0:0adc2171, 10K
D250 p0|01 ???[??-00]:SEP  PMCSIERA SRC 8x6G       ,RevC,WWID=50014380:07e874ef
D251 p0|01 ???[??-00]:SGPIO                        ,    ,WWID=50014380:07e874e0
D253                 :Protocol Adapter
D254                 :Protocol Adapter
Total Discovered SAS  Devices:  3

*****  Onboard PHY Link Rates  ****
   \PHYS         0          10         20         30         40
Onboard Phys   : AAA00000

*****  Expander PHY Link Rates  ****
EXP\PHYS         0          10         20         30         40
Total 6.0G Links:  3
DirtyQMemBytes: 147456
Local Memory Avail      7772092 bytes in 43 fragments
Shared Memory Avail     8367492 bytes in 17 fragments
Logical Reqs Avail      1023
Physical Reqs Avail     1020
Host Prefetch is ENABLED
ROM Flash Driver Init Passed
Testing ROM Image A
Testing ROM Image B
PCI rev. 0x1 using 4 lanes @5.0G

Host-to-local data xfer rate, using CPU:  571 MB/sec
Host-to-local data xfer rate, using DMA:  1384 MB/sec
Host time is 1:09:48, 4/24/2011
PCI slot 0
Periodic iLO command check interval=1 seconds, hostaddr=0x0DF63E020.
Host time is 1:09:50, 4/24/2011
PCI slot 0

[04/24 01:09:50]

Run-Time LF: DIS: 0x00, SL_SAS: 0x00, SL_SATA: 0x00, LFV: 0x03, PBP: 0xff

[04/24 01:09:53]Local-to-host data xfer rate, using DMA:  1445 MB/sec
[04/24 01:09:53]Int13 BIOS unit 0x80 = CISS LUN 0x4000000000000000 


Copyright (C) HP Corporation 1990-2010.
All rights reserved.
HP Array Controller Firmware Ver = 3.00, Build Num = 0
   BootBlock Ver = 2.07, HAL-PL Ver = 02.03.011.001
Compiled Feb 17 2010 14:42:36

PASSED: HAL API Initialization
FirstAvail : 0x80a1be40


Initializing Memory...

Physical Requests    1407
Logical Requests     1024
Command Lists        1025
Local Memory Avail      10735376 bytes in 5 fragments
Shared Memory Avail     8388600 bytes in 2 fragments
Logical Reqs Avail      1024
Physical Reqs Avail     1407
Host Prefetch is ENABLED
PASSED: Memory Initialization

SSID = 3245103c
PASSED: I2C Initialization

NVRAM Update: ILA returned 0x0
PASSED: Bootstrap NVRAM Checksum

Platform NVRAM auto-update found an embedded image, but it is not an upgrade

PASSED: Command I/O Initialization
PASSED: Timer Initialization

Board is Marble     Rev. C
Using WWID to generate new board serial #: 5001438007E874E
NumMgmtDevices = 105 MgmtDeviceStartIndex = 146
num_drive_params_entries = 255 drive params size = 49980

Diagnostic Pointers Initialized
Diagnostic download address = 0x817e8000
Initializing XOR Engine...
validate_pic_fw: pic version in ROM = 52
Battery 1 not present.
Battery 2 not present.
Battery 3 not present.

Battery Status:    Battery 1      Battery 2      Battery 3
---------------    ---------      ---------      ---------
Present:               NO             NO             NO
Responding:           N/A            N/A            N/A


Found 256 MB of cache memory.
wcxc_ram_start = 0x47000000
wcxc_ram_size  = 0x09000000
DIMM SN: PACCQ9SYWI29
Initializing ADG for SAS controllers only (tolerate 8 drive failure)
ADG keys initialized

Starting DMA SelfTest
   Pattern Fill DMA mem write xfer rate:         1669 MB/sec
   Pattern Fill DMA mem read xfer rate:          1873 MB/sec
   Zero Pattern Fill DMA mem write xfer rate:    1668 MB/sec
   Zero Pattern Fill DMA mem read xfer rate:     1872 MB/sec
   Mem-to-mem DMA xfer rate:                     914 MB/sec
   Mem-to-WXOR DMA xfer rate:                    617 MB/sec
   Mem-to-WXOR Multicast xfer rate:              795 MB/sec
   Mem-to-Mem DMA_SendCDB xfer rate:             161 MB/sec
   Mem-to-Mem DMA_SendCDB w/XOR xfer rate:       165 MB/sec
ADG SelfTestOK

PASSED: DMAXOR Controller Initialization

PASSED: Cache Controller Initialization

PAL_CO_Init: tbl_entries = 255 size = 142800
Start Up Complete
Memory start 47000000
Memory size 9000000
Cache Mem Test PASSED!


Pre-discovery LF: DIS: 0x00, SL_SAS: 0x00, SL_SATA: 0x00, LFV: 0x03, PBP: 0xff

Protocol device 0 scan devices started
Protocol device 0 scan devices done
Adapter 0 Bus Reset
PR 80aa10b8h:D000 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:02
PR 80aa10b8h:D001 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:02
PR 80aa10b8h:D002 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:02
PR 80aa10b8h:D250 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
get_drive_params: Inquiry to SEP for VPD page to get serial # failed.
Updated full box tbl in RIS

Configured logical unit (volume) count = 1
   ccf=0x00, mccf=0x00000000
Array A Unit 0: RAID 5; df=128 vs=OK drvs=3 dd=2 pg=1 vofs=0x000000000 blks=0x0222CE330 ca=ena srf=0x1 dt=2
  U0 drive map (hex) = 00 01 02
Controller WWID = 5001438007e874e0

*****  Discovered SAS (Compatible) Devices  ****
D000 p0|01 P1I[00-01]:Disk HP      DG0146FARVU     ,HPD8,WWID=5000cca0:0adf7b79, 10K
D001 p0|01 P1I[00-02]:Disk HP      DG0146FARVU     ,HPD8,WWID=5000cca0:0ae013c1, 10K
D002 p0|01 P1I[00-03]:Disk HP      DG0146FARVU     ,HPD8,WWID=5000cca0:0adc2171, 10K
D250 p0|01 ???[??-00]:SEP  PMCSIERA SRC 8x6G       ,RevC,WWID=50014380:07e874ef
D251 p0|01 ???[??-00]:SGPIO                        ,    ,WWID=50014380:07e874e0
D253                 :Protocol Adapter
D254                 :Protocol Adapter
Total Discovered SAS  Devices:  3

*****  Onboard PHY Link Rates  ****
   \PHYS         0          10         20         30         40
Onboard Phys   : AAA00000

*****  Expander PHY Link Rates  ****
EXP\PHYS         0          10         20         30         40
Total 6.0G Links:  3
DirtyQMemBytes: 147456
Local Memory Avail      7772092 bytes in 43 fragments
Shared Memory Avail     8367492 bytes in 17 fragments
Logical Reqs Avail      1023
Physical Reqs Avail     1020
Host Prefetch is ENABLED
ROM Flash Driver Init Passed
Testing ROM Image A
Testing ROM Image B
PCI rev. 0x1 using 4 lanes @5.0G

Host-to-local data xfer rate, using CPU:  650 MB/sec
Host-to-local data xfer rate, using DMA:  1402 MB/sec
Host time is 1:41:02, 4/24/2011
PCI slot 0
Periodic iLO command check interval=1 seconds, hostaddr=0x0DF63E020.
Host time is 1:41:05, 4/24/2011
PCI slot 0

[04/24 01:41:05]

Run-Time LF: DIS: 0x00, SL_SAS: 0x00, SL_SATA: 0x00, LFV: 0x03, PBP: 0xff

[04/24 01:41:08]Local-to-host data xfer rate, using DMA:  1368 MB/sec
[04/24 01:41:08]Int13 BIOS unit 0x80 = CISS LUN 0x4000000000000000 


Copyright (C) HP Corporation 1990-2010.
All rights reserved.
HP Array Controller Firmware Ver = 3.00, Build Num = 0
   BootBlock Ver = 2.07, HAL-PL Ver = 02.03.011.001
Compiled Feb 17 2010 14:42:36

PASSED: HAL API Initialization
FirstAvail : 0x80a1be40


Initializing Memory...

Physical Requests    1407
Logical Requests     1024
Command Lists        1025
Local Memory Avail      10735376 bytes in 5 fragments
Shared Memory Avail     8388600 bytes in 2 fragments
Logical Reqs Avail      1024
Physical Reqs Avail     1407
Host Prefetch is ENABLED
PASSED: Memory Initialization

SSID = 3245103c
PASSED: I2C Initialization

NVRAM Update: ILA returned 0x0
PASSED: Bootstrap NVRAM Checksum

Platform NVRAM auto-update found an embedded image, but it is not an upgrade

PASSED: Command I/O Initialization
PASSED: Timer Initialization

Board is Marble     Rev. C
Using WWID to generate new board serial #: 5001438007E874E
NumMgmtDevices = 105 MgmtDeviceStartIndex = 146
num_drive_params_entries = 255 drive params size = 49980

Diagnostic Pointers Initialized
Diagnostic download address = 0x817e8000
Initializing XOR Engine...
validate_pic_fw: pic version in ROM = 52
Battery 1 not present.
Battery 2 not present.
Battery 3 not present.

Battery Status:    Battery 1      Battery 2      Battery 3
---------------    ---------      ---------      ---------
Present:               NO             NO             NO
Responding:           N/A            N/A            N/A


Found 256 MB of cache memory.
wcxc_ram_start = 0x47000000
wcxc_ram_size  = 0x09000000
DIMM SN: PACCQ9SYWI29
Initializing ADG for SAS controllers only (tolerate 8 drive failure)
ADG keys initialized

Starting DMA SelfTest
   Pattern Fill DMA mem write xfer rate:         1671 MB/sec
   Pattern Fill DMA mem read xfer rate:          1873 MB/sec
   Zero Pattern Fill DMA mem write xfer rate:    1669 MB/sec
   Zero Pattern Fill DMA mem read xfer rate:     1873 MB/sec
   Mem-to-mem DMA xfer rate:                     910 MB/sec
   Mem-to-WXOR DMA xfer rate:                    615 MB/sec
   Mem-to-WXOR Multicast xfer rate:              795 MB/sec
   Mem-to-Mem DMA_SendCDB xfer rate:             163 MB/sec
   Mem-to-Mem DMA_SendCDB w/XOR xfer rate:       180 MB/sec
ADG SelfTestOK

PASSED: DMAXOR Controller Initialization

PASSED: Cache Controller Initialization

PAL_CO_Init: tbl_entries = 255 size = 142800
Start Up Complete
Memory start 47000000
Memory size 9000000
Cache Mem Test PASSED!


Pre-discovery LF: DIS: 0x00, SL_SAS: 0x00, SL_SATA: 0x00, LFV: 0x03, PBP: 0xff

Protocol device 0 scan devices started
Protocol device 0 scan devices done
Adapter 0 Bus Reset
PR 80aa10b8h:D000 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:02
PR 80aa10b8h:D001 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:02
PR 80aa10b8h:D002 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:02
PR 80aa10b8h:D250 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
get_drive_params: Inquiry to SEP for VPD page to get serial # failed.
Updated full box tbl in RIS

Configured logical unit (volume) count = 1
   ccf=0x00, mccf=0x00000000
Array A Unit 0: RAID 5; df=128 vs=OK drvs=3 dd=2 pg=1 vofs=0x000000000 blks=0x0222CE330 ca=ena srf=0x1 dt=2
  U0 drive map (hex) = 00 01 02
Controller WWID = 5001438007e874e0

*****  Discovered SAS (Compatible) Devices  ****
D000 p0|01 P1I[00-01]:Disk HP      DG0146FARVU     ,HPD8,WWID=5000cca0:0adf7b79, 10K
D001 p0|01 P1I[00-02]:Disk HP      DG0146FARVU     ,HPD8,WWID=5000cca0:0ae013c1, 10K
D002 p0|01 P1I[00-03]:Disk HP      DG0146FARVU     ,HPD8,WWID=5000cca0:0adc2171, 10K
D250 p0|01 ???[??-00]:SEP  PMCSIERA SRC 8x6G       ,RevC,WWID=50014380:07e874ef
D251 p0|01 ???[??-00]:SGPIO                        ,    ,WWID=50014380:07e874e0
D253                 :Protocol Adapter
D254                 :Protocol Adapter
Total Discovered SAS  Devices:  3

*****  Onboard PHY Link Rates  ****
   \PHYS         0          10         20         30         40
Onboard Phys   : AAA00000

*****  Expander PHY Link Rates  ****
EXP\PHYS         0          10         20         30         40
Total 6.0G Links:  3
DirtyQMemBytes: 147456
Local Memory Avail      7772092 bytes in 43 fragments
Shared Memory Avail     8367492 bytes in 17 fragments
Logical Reqs Avail      1023
Physical Reqs Avail     1020
Host Prefetch is ENABLED
ROM Flash Driver Init Passed
Testing ROM Image A
Testing ROM Image B
PCI rev. 0x1 using 4 lanes @5.0G

Host-to-local data xfer rate, using CPU:  587 MB/sec
Host-to-local data xfer rate, using DMA:  1379 MB/sec
Host time is 23:48:39, 4/24/2011
PCI slot 0
Periodic iLO command check interval=1 seconds, hostaddr=0x0DF63E020.
Host time is 23:48:41, 4/24/2011
PCI slot 0

[04/24 23:48:41]

Run-Time LF: DIS: 0x00, SL_SAS: 0x00, SL_SATA: 0x00, LFV: 0x03, PBP: 0xff

[04/24 23:48:44]Local-to-host data xfer rate, using DMA:  1459 MB/sec
[04/24 23:48:44]Int13 BIOS unit 0x80 = CISS LUN 0x4000000000000000 


Copyright (C) HP Corporation 1990-2010.
All rights reserved.
HP Array Controller Firmware Ver = 3.00, Build Num = 0
   BootBlock Ver = 2.07, HAL-PL Ver = 02.03.011.001
Compiled Feb 17 2010 14:42:36

PASSED: HAL API Initialization
FirstAvail : 0x80a1be40


Initializing Memory...

Physical Requests    1407
Logical Requests     1024
Command Lists        1025
Local Memory Avail      10735376 bytes in 5 fragments
Shared Memory Avail     8388600 bytes in 2 fragments
Logical Reqs Avail      1024
Physical Reqs Avail     1407
Host Prefetch is ENABLED
PASSED: Memory Initialization

SSID = 3245103c
PASSED: I2C Initialization

NVRAM Update: ILA returned 0x0
PASSED: Bootstrap NVRAM Checksum

Platform NVRAM auto-update found an embedded image, but it is not an upgrade

PASSED: Command I/O Initialization
PASSED: Timer Initialization

Board is Marble     Rev. C
Using WWID to generate new board serial #: 5001438007E874E
NumMgmtDevices = 105 MgmtDeviceStartIndex = 146
num_drive_params_entries = 255 drive params size = 49980

Diagnostic Pointers Initialized
Diagnostic download address = 0x817e8000
Initializing XOR Engine...
validate_pic_fw: pic version in ROM = 52
Battery 1 not present.
Battery 2 not present.
Battery 3 not present.

Battery Status:    Battery 1      Battery 2      Battery 3
---------------    ---------      ---------      ---------
Present:               NO             NO             NO
Responding:           N/A            N/A            N/A


Found 256 MB of cache memory.
wcxc_ram_start = 0x47000000
wcxc_ram_size  = 0x09000000
DIMM SN: PACCQ9SYWI29
Initializing ADG for SAS controllers only (tolerate 8 drive failure)
ADG keys initialized

Starting DMA SelfTest
   Pattern Fill DMA mem write xfer rate:         1671 MB/sec
   Pattern Fill DMA mem read xfer rate:          1872 MB/sec
   Zero Pattern Fill DMA mem write xfer rate:    1669 MB/sec
   Zero Pattern Fill DMA mem read xfer rate:     1872 MB/sec
   Mem-to-mem DMA xfer rate:                     911 MB/sec
   Mem-to-WXOR DMA xfer rate:                    612 MB/sec
   Mem-to-WXOR Multicast xfer rate:              793 MB/sec
   Mem-to-Mem DMA_SendCDB xfer rate:             166 MB/sec
   Mem-to-Mem DMA_SendCDB w/XOR xfer rate:       180 MB/sec
ADG SelfTestOK

PASSED: DMAXOR Controller Initialization

PASSED: Cache Controller Initialization

PAL_CO_Init: tbl_entries = 255 size = 142800
Start Up Complete
Memory start 47000000
Memory size 9000000
Cache Mem Test PASSED!


Pre-discovery LF: DIS: 0x00, SL_SAS: 0x00, SL_SATA: 0x00, LFV: 0x03, PBP: 0xff

Protocol device 0 scan devices started
Protocol device 0 scan devices done
Adapter 0 Bus Reset
PR 80aa10b8h:D000 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:02
PR 80aa10b8h:D001 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:02
PR 80aa10b8h:D002 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:02
PR 80aa10b8h:D250 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
get_drive_params: Inquiry to SEP for VPD page to get serial # failed.
Updated full box tbl in RIS

Configured logical unit (volume) count = 1
   ccf=0x00, mccf=0x00000000
Array A Unit 0: RAID 5; df=128 vs=OK drvs=3 dd=2 pg=1 vofs=0x000000000 blks=0x0222CE330 ca=ena srf=0x1 dt=2
  U0 drive map (hex) = 00 01 02
Controller WWID = 5001438007e874e0

*****  Discovered SAS (Compatible) Devices  ****
D000 p0|01 P1I[00-01]:Disk HP      DG0146FARVU     ,HPD8,WWID=5000cca0:0adf7b79, 10K
D001 p0|01 P1I[00-02]:Disk HP      DG0146FARVU     ,HPD8,WWID=5000cca0:0ae013c1, 10K
D002 p0|01 P1I[00-03]:Disk HP      DG0146FARVU     ,HPD8,WWID=5000cca0:0adc2171, 10K
D250 p0|01 ???[??-00]:SEP  PMCSIERA SRC 8x6G       ,RevC,WWID=50014380:07e874ef
D251 p0|01 ???[??-00]:SGPIO                        ,    ,WWID=50014380:07e874e0
D253                 :Protocol Adapter
D254                 :Protocol Adapter
Total Discovered SAS  Devices:  3

*****  Onboard PHY Link Rates  ****
   \PHYS         0          10         20         30         40
Onboard Phys   : AAA00000

*****  Expander PHY Link Rates  ****
EXP\PHYS         0          10         20         30         40
Total 6.0G Links:  3
DirtyQMemBytes: 147456
Local Memory Avail      7772092 bytes in 43 fragments
Shared Memory Avail     8367492 bytes in 17 fragments
Logical Reqs Avail      1023
Physical Reqs Avail     1020
Host Prefetch is ENABLED
ROM Flash Driver Init Passed
Testing ROM Image A
Testing ROM Image B
PCI rev. 0x1 using 4 lanes @5.0G

Host-to-local data xfer rate, using CPU:  570 MB/sec
Host-to-local data xfer rate, using DMA:  1384 MB/sec
Host time is 19:51:42, 4/26/2011
PCI slot 0
Periodic iLO command check interval=1 seconds, hostaddr=0x0DF63E020.
Host time is 19:51:43, 4/26/2011
PCI slot 0

[04/26 19:51:43]

Run-Time LF: DIS: 0x00, SL_SAS: 0x00, SL_SATA: 0x00, LFV: 0x03, PBP: 0xff

[04/26 19:51:46]Local-to-host data xfer rate, using DMA:  1455 MB/sec
[04/26 19:51:46]Int13 BIOS unit 0x80 = CISS LUN 0x4000000000000000 


Copyright (C) HP Corporation 1990-2010.
All rights reserved.
HP Array Controller Firmware Ver = 3.00, Build Num = 0
   BootBlock Ver = 2.07, HAL-PL Ver = 02.03.011.001
Compiled Feb 17 2010 14:42:36

PASSED: HAL API Initialization
FirstAvail : 0x80a1be40


Initializing Memory...

Physical Requests    1407
Logical Requests     1024
Command Lists        1025
Local Memory Avail      10735376 bytes in 5 fragments
Shared Memory Avail     8388600 bytes in 2 fragments
Logical Reqs Avail      1024
Physical Reqs Avail     1407
Host Prefetch is ENABLED
PASSED: Memory Initialization

SSID = 3245103c
PASSED: I2C Initialization

NVRAM Update: ILA returned 0x0
PASSED: Bootstrap NVRAM Checksum

Platform NVRAM auto-update found an embedded image, but it is not an upgrade

PASSED: Command I/O Initialization
PASSED: Timer Initialization

Board is Marble     Rev. C
Using WWID to generate new board serial #: 5001438007E874E
NumMgmtDevices = 105 MgmtDeviceStartIndex = 146
num_drive_params_entries = 255 drive params size = 49980

Diagnostic Pointers Initialized
Diagnostic download address = 0x817e8000
Initializing XOR Engine...
validate_pic_fw: pic version in ROM = 52
Battery 1 not present.
Battery 2 not present.
Battery 3 not present.

Battery Status:    Battery 1      Battery 2      Battery 3
---------------    ---------      ---------      ---------
Present:               NO             NO             NO
Responding:           N/A            N/A            N/A


Found 256 MB of cache memory.
wcxc_ram_start = 0x47000000
wcxc_ram_size  = 0x09000000
DIMM SN: PACCQ9SYWI29
Initializing ADG for SAS controllers only (tolerate 8 drive failure)
ADG keys initialized

Starting DMA SelfTest
   Pattern Fill DMA mem write xfer rate:         1670 MB/sec
   Pattern Fill DMA mem read xfer rate:          1873 MB/sec
   Zero Pattern Fill DMA mem write xfer rate:    1668 MB/sec
   Zero Pattern Fill DMA mem read xfer rate:     1873 MB/sec
   Mem-to-mem DMA xfer rate:                     910 MB/sec
   Mem-to-WXOR DMA xfer rate:                    630 MB/sec
   Mem-to-WXOR Multicast xfer rate:              802 MB/sec
   Mem-to-Mem DMA_SendCDB xfer rate:             165 MB/sec
   Mem-to-Mem DMA_SendCDB w/XOR xfer rate:       165 MB/sec
ADG SelfTestOK

PASSED: DMAXOR Controller Initialization

PASSED: Cache Controller Initialization

PAL_CO_Init: tbl_entries = 255 size = 142800
Start Up Complete
Memory start 47000000
Memory size 9000000
Cache Mem Test PASSED!


Pre-discovery LF: DIS: 0x00, SL_SAS: 0x00, SL_SATA: 0x00, LFV: 0x03, PBP: 0xff

Protocol device 0 scan devices started
Protocol device 0 scan devices done
Adapter 0 Bus Reset
PR 80aa10b8h:D000 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:02
PR 80aa10b8h:D001 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:02
PR 80aa10b8h:D002 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:02
PR 80aa10b8h:D250 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
get_drive_params: Inquiry to SEP for VPD page to get serial # failed.
Updated full box tbl in RIS

Configured logical unit (volume) count = 1
   ccf=0x00, mccf=0x00000000
Array A Unit 0: RAID 5; df=128 vs=OK drvs=3 dd=2 pg=1 vofs=0x000000000 blks=0x0222CE330 ca=ena srf=0x1 dt=2
  U0 drive map (hex) = 00 01 02
Controller WWID = 5001438007e874e0

*****  Discovered SAS (Compatible) Devices  ****
D000 p0|01 P1I[00-01]:Disk HP      DG0146FARVU     ,HPD8,WWID=5000cca0:0adf7b79, 10K
D001 p0|01 P1I[00-02]:Disk HP      DG0146FARVU     ,HPD8,WWID=5000cca0:0ae013c1, 10K
D002 p0|01 P1I[00-03]:Disk HP      DG0146FARVU     ,HPD8,WWID=5000cca0:0adc2171, 10K
D250 p0|01 ???[??-00]:SEP  PMCSIERA SRC 8x6G       ,RevC,WWID=50014380:07e874ef
D251 p0|01 ???[??-00]:SGPIO                        ,    ,WWID=50014380:07e874e0
D253                 :Protocol Adapter
D254                 :Protocol Adapter
Total Discovered SAS  Devices:  3

*****  Onboard PHY Link Rates  ****
   \PHYS         0          10         20         30         40
Onboard Phys   : AAA00000

*****  Expander PHY Link Rates  ****
EXP\PHYS         0          10         20         30         40
Total 6.0G Links:  3
DirtyQMemBytes: 147456
Local Memory Avail      7772092 bytes in 43 fragments
Shared Memory Avail     8367492 bytes in 17 fragments
Logical Reqs Avail      1023
Physical Reqs Avail     1020
Host Prefetch is ENABLED
ROM Flash Driver Init Passed
Testing ROM Image A
Testing ROM Image B
PCI rev. 0x1 using 4 lanes @5.0G

Host-to-local data xfer rate, using CPU:  653 MB/sec
Host-to-local data xfer rate, using DMA:  1402 MB/sec
Host time is 16:30:50, 5/09/2011
PCI slot 0
Periodic iLO command check interval=1 seconds, hostaddr=0x0DF63E020.
Host time is 16:30:52, 5/09/2011
PCI slot 0

[05/09 16:30:52]

Run-Time LF: DIS: 0x00, SL_SAS: 0x00, SL_SATA: 0x00, LFV: 0x03, PBP: 0xff

[05/09 16:30:55]Local-to-host data xfer rate, using DMA:  1464 MB/sec
[05/09 16:30:55]Int13 BIOS unit 0x80 = CISS LUN 0x4000000000000000 


Copyright (C) HP Corporation 1990-2010.
All rights reserved.
HP Array Controller Firmware Ver = 3.00, Build Num = 0
   BootBlock Ver = 2.07, HAL-PL Ver = 02.03.011.001
Compiled Feb 17 2010 14:42:36

PASSED: HAL API Initialization
FirstAvail : 0x80a1be40


Initializing Memory...

Physical Requests    1407
Logical Requests     1024
Command Lists        1025
Local Memory Avail      10735376 bytes in 5 fragments
Shared Memory Avail     8388600 bytes in 2 fragments
Logical Reqs Avail      1024
Physical Reqs Avail     1407
Host Prefetch is ENABLED
PASSED: Memory Initialization

SSID = 3245103c
PASSED: I2C Initialization

NVRAM Update: ILA returned 0x0
PASSED: Bootstrap NVRAM Checksum

Platform NVRAM auto-update found an embedded image, but it is not an upgrade

PASSED: Command I/O Initialization
PASSED: Timer Initialization

Board is Marble     Rev. C
Using WWID to generate new board serial #: 5001438007E874E
NumMgmtDevices = 105 MgmtDeviceStartIndex = 146
num_drive_params_entries = 255 drive params size = 49980

Diagnostic Pointers Initialized
Diagnostic download address = 0x817e8000
Initializing XOR Engine...
validate_pic_fw: pic version in ROM = 52
Battery 1 not present.
Battery 2 not present.
Battery 3 not present.

Battery Status:    Battery 1      Battery 2      Battery 3
---------------    ---------      ---------      ---------
Present:               NO             NO             NO
Responding:           N/A            N/A            N/A


Found 256 MB of cache memory.
wcxc_ram_start = 0x47000000
wcxc_ram_size  = 0x09000000
DIMM SN: PACCQ9SYWI29
Initializing ADG for SAS controllers only (tolerate 8 drive failure)
ADG keys initialized

Starting DMA SelfTest
   Pattern Fill DMA mem write xfer rate:         1671 MB/sec
   Pattern Fill DMA mem read xfer rate:          1875 MB/sec
   Zero Pattern Fill DMA mem write xfer rate:    1667 MB/sec
   Zero Pattern Fill DMA mem read xfer rate:     1872 MB/sec
   Mem-to-mem DMA xfer rate:                     909 MB/sec
   Mem-to-WXOR DMA xfer rate:                    616 MB/sec
   Mem-to-WXOR Multicast xfer rate:              791 MB/sec
   Mem-to-Mem DMA_SendCDB xfer rate:             168 MB/sec
   Mem-to-Mem DMA_SendCDB w/XOR xfer rate:       180 MB/sec
ADG SelfTestOK

PASSED: DMAXOR Controller Initialization

PASSED: Cache Controller Initialization

PAL_CO_Init: tbl_entries = 255 size = 142800
Start Up Complete
Memory start 47000000
Memory size 9000000
Cache Mem Test PASSED!


Pre-discovery LF: DIS: 0x00, SL_SAS: 0x00, SL_SATA: 0x00, LFV: 0x03, PBP: 0xff

Protocol device 0 scan devices started
Protocol device 0 scan devices done
Adapter 0 Bus Reset
PR 80aa10b8h:D000 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:02
PR 80aa10b8h:D001 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:02
PR 80aa10b8h:D002 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:02
PR 80aa10b8h:D250 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
get_drive_params: Inquiry to SEP for VPD page to get serial # failed.
Updated full box tbl in RIS

Configured logical unit (volume) count = 1
   ccf=0x00, mccf=0x00000000
Array A Unit 0: RAID 5; df=128 vs=OK drvs=3 dd=2 pg=1 vofs=0x000000000 blks=0x0222CE330 ca=ena srf=0x1 dt=2
  U0 drive map (hex) = 00 01 02
Controller WWID = 5001438007e874e0

*****  Discovered SAS (Compatible) Devices  ****
D000 p0|01 P1I[00-01]:Disk HP      DG0146FARVU     ,HPD8,WWID=5000cca0:0adf7b79, 10K
D001 p0|01 P1I[00-02]:Disk HP      DG0146FARVU     ,HPD8,WWID=5000cca0:0ae013c1, 10K
D002 p0|01 P1I[00-03]:Disk HP      DG0146FARVU     ,HPD8,WWID=5000cca0:0adc2171, 10K
D250 p0|01 ???[??-00]:SEP  PMCSIERA SRC 8x6G       ,RevC,WWID=50014380:07e874ef
D251 p0|01 ???[??-00]:SGPIO                        ,    ,WWID=50014380:07e874e0
D253                 :Protocol Adapter
D254                 :Protocol Adapter
Total Discovered SAS  Devices:  3

*****  Onboard PHY Link Rates  ****
   \PHYS         0          10         20         30         40
Onboard Phys   : AAA00000

*****  Expander PHY Link Rates  ****
EXP\PHYS         0          10         20         30         40
Total 6.0G Links:  3
DirtyQMemBytes: 147456
Local Memory Avail      7772092 bytes in 43 fragments
Shared Memory Avail     8367492 bytes in 17 fragments
Logical Reqs Avail      1023
Physical Reqs Avail     1020
Host Prefetch is ENABLED
ROM Flash Driver Init Passed
Testing ROM Image A
Testing ROM Image B
PCI rev. 0x1 using 4 lanes @5.0G

Host-to-local data xfer rate, using CPU:  637 MB/sec
Host-to-local data xfer rate, using DMA:  1395 MB/sec
Host time is 22:37:23, 5/13/2011
PCI slot 0
Periodic iLO command check interval=1 seconds, hostaddr=0x0DF63E020.
Host time is 22:37:25, 5/13/2011
PCI slot 0

[05/13 22:37:25]

Run-Time LF: DIS: 0x00, SL_SAS: 0x00, SL_SATA: 0x00, LFV: 0x03, PBP: 0xff

[05/13 22:37:28]Local-to-host data xfer rate, using DMA:  1449 MB/sec
[05/13 22:37:28]Int13 BIOS unit 0x80 = CISS LUN 0x4000000000000000 


Copyright (C) HP Corporation 1990-2010.
All rights reserved.
HP Array Controller Firmware Ver = 3.00, Build Num = 0
   BootBlock Ver = 2.07, HAL-PL Ver = 02.03.011.001
Compiled Feb 17 2010 14:42:36

PASSED: HAL API Initialization
FirstAvail : 0x80a1be40


Initializing Memory...

Physical Requests    1407
Logical Requests     1024
Command Lists        1025
Local Memory Avail      10735376 bytes in 5 fragments
Shared Memory Avail     8388600 bytes in 2 fragments
Logical Reqs Avail      1024
Physical Reqs Avail     1407
Host Prefetch is ENABLED
PASSED: Memory Initialization

SSID = 3245103c
PASSED: I2C Initialization

NVRAM Update: ILA returned 0x0
PASSED: Bootstrap NVRAM Checksum

Platform NVRAM auto-update found an embedded image, but it is not an upgrade

PASSED: Command I/O Initialization
PASSED: Timer Initialization

Board is Marble     Rev. C
Using WWID to generate new board serial #: 5001438007E874E
NumMgmtDevices = 105 MgmtDeviceStartIndex = 146
num_drive_params_entries = 255 drive params size = 49980

Diagnostic Pointers Initialized
Diagnostic download address = 0x817e8000
Initializing XOR Engine...
validate_pic_fw: pic version in ROM = 52
Battery 1 not present.
Battery 2 not present.
Battery 3 not present.

Battery Status:    Battery 1      Battery 2      Battery 3
---------------    ---------      ---------      ---------
Present:               NO             NO             NO
Responding:           N/A            N/A            N/A


Found 256 MB of cache memory.
wcxc_ram_start = 0x47000000
wcxc_ram_size  = 0x09000000
DIMM SN: PACCQ9SYWI29
Initializing ADG for SAS controllers only (tolerate 8 drive failure)
ADG keys initialized

Starting DMA SelfTest
   Pattern Fill DMA mem write xfer rate:         1672 MB/sec
   Pattern Fill DMA mem read xfer rate:          1872 MB/sec
   Zero Pattern Fill DMA mem write xfer rate:    1669 MB/sec
   Zero Pattern Fill DMA mem read xfer rate:     1873 MB/sec
   Mem-to-mem DMA xfer rate:                     906 MB/sec
   Mem-to-WXOR DMA xfer rate:                    625 MB/sec
   Mem-to-WXOR Multicast xfer rate:              791 MB/sec
   Mem-to-Mem DMA_SendCDB xfer rate:             168 MB/sec
   Mem-to-Mem DMA_SendCDB w/XOR xfer rate:       180 MB/sec
ADG SelfTestOK

PASSED: DMAXOR Controller Initialization

PASSED: Cache Controller Initialization

PAL_CO_Init: tbl_entries = 255 size = 142800
Start Up Complete
Memory start 47000000
Memory size 9000000
Cache Mem Test PASSED!


Pre-discovery LF: DIS: 0x00, SL_SAS: 0x00, SL_SATA: 0x00, LFV: 0x03, PBP: 0xff

Protocol device 0 scan devices started
Protocol device 0 scan devices done
Adapter 0 Bus Reset
PR 80aa10b8h:D000 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:02
PR 80aa10b8h:D001 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:02
PR 80aa10b8h:D002 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:02
PR 80aa10b8h:D250 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
get_drive_params: Inquiry to SEP for VPD page to get serial # failed.
Updated full box tbl in RIS

Configured logical unit (volume) count = 1
   ccf=0x00, mccf=0x00000000
Array A Unit 0: RAID 5; df=128 vs=OK drvs=3 dd=2 pg=1 vofs=0x000000000 blks=0x0222CE330 ca=ena srf=0x1 dt=2
  U0 drive map (hex) = 00 01 02
Controller WWID = 5001438007e874e0

*****  Discovered SAS (Compatible) Devices  ****
D000 p0|01 P1I[00-01]:Disk HP      DG0146FARVU     ,HPD8,WWID=5000cca0:0adf7b79, 10K
D001 p0|01 P1I[00-02]:Disk HP      DG0146FARVU     ,HPD8,WWID=5000cca0:0ae013c1, 10K
D002 p0|01 P1I[00-03]:Disk HP      DG0146FARVU     ,HPD8,WWID=5000cca0:0adc2171, 10K
D250 p0|01 ???[??-00]:SEP  PMCSIERA SRC 8x6G       ,RevC,WWID=50014380:07e874ef
D251 p0|01 ???[??-00]:SGPIO                        ,    ,WWID=50014380:07e874e0
D253                 :Protocol Adapter
D254                 :Protocol Adapter
Total Discovered SAS  Devices:  3

*****  Onboard PHY Link Rates  ****
   \PHYS         0          10         20         30         40
Onboard Phys   : AAA00000

*****  Expander PHY Link Rates  ****
EXP\PHYS         0          10         20         30         40
Total 6.0G Links:  3
DirtyQMemBytes: 147456
Local Memory Avail      7772092 bytes in 43 fragments
Shared Memory Avail     8367492 bytes in 17 fragments
Logical Reqs Avail      1023
Physical Reqs Avail     1020
Host Prefetch is ENABLED
ROM Flash Driver Init Passed
Testing ROM Image A
Testing ROM Image B
PCI rev. 0x1 using 4 lanes @5.0G

Host-to-local data xfer rate, using CPU:  586 MB/sec
Host-to-local data xfer rate, using DMA:  1384 MB/sec
Host time is 15:03:19, 5/14/2011
PCI slot 0
Periodic iLO command check interval=1 seconds, hostaddr=0x0DF63E020.
Host time is 15:03:21, 5/14/2011
PCI slot 0

[05/14 15:03:21]

Run-Time LF: DIS: 0x00, SL_SAS: 0x00, SL_SATA: 0x00, LFV: 0x03, PBP: 0xff

[05/14 15:03:24]Local-to-host data xfer rate, using DMA:  1445 MB/sec
[05/14 15:03:24]Int13 BIOS unit 0x80 = CISS LUN 0x4000000000000000 


Copyright (C) HP Corporation 1990-2010.
All rights reserved.
HP Array Controller Firmware Ver = 3.00, Build Num = 0
   BootBlock Ver = 2.07, HAL-PL Ver = 02.03.011.001
Compiled Feb 17 2010 14:42:36

PASSED: HAL API Initialization
FirstAvail : 0x80a1be40


Initializing Memory...

Physical Requests    1407
Logical Requests     1024
Command Lists        1025
Local Memory Avail      10735376 bytes in 5 fragments
Shared Memory Avail     8388600 bytes in 2 fragments
Logical Reqs Avail      1024
Physical Reqs Avail     1407
Host Prefetch is ENABLED
PASSED: Memory Initialization

SSID = 3245103c
PASSED: I2C Initialization

NVRAM Update: ILA returned 0x0
PASSED: Bootstrap NVRAM Checksum

Platform NVRAM auto-update found an embedded image, but it is not an upgrade

PASSED: Command I/O Initialization
PASSED: Timer Initialization

Board is Marble     Rev. C
Using WWID to generate new board serial #: 5001438007E874E
NumMgmtDevices = 105 MgmtDeviceStartIndex = 146
num_drive_params_entries = 255 drive params size = 49980

Diagnostic Pointers Initialized
Diagnostic download address = 0x817e8000
Initializing XOR Engine...
validate_pic_fw: pic version in ROM = 52
Battery 1 not present.
Battery 2 not present.
Battery 3 not present.

Battery Status:    Battery 1      Battery 2      Battery 3
---------------    ---------      ---------      ---------
Present:               NO             NO             NO
Responding:           N/A            N/A            N/A


Found 256 MB of cache memory.
wcxc_ram_start = 0x47000000
wcxc_ram_size  = 0x09000000
DIMM SN: PACCQ9SYWI29
Initializing ADG for SAS controllers only (tolerate 8 drive failure)
ADG keys initialized

Starting DMA SelfTest
   Pattern Fill DMA mem write xfer rate:         1670 MB/sec
   Pattern Fill DMA mem read xfer rate:          1872 MB/sec
   Zero Pattern Fill DMA mem write xfer rate:    1668 MB/sec
   Zero Pattern Fill DMA mem read xfer rate:     1872 MB/sec
   Mem-to-mem DMA xfer rate:                     911 MB/sec
   Mem-to-WXOR DMA xfer rate:                    617 MB/sec
   Mem-to-WXOR Multicast xfer rate:              791 MB/sec
   Mem-to-Mem DMA_SendCDB xfer rate:             166 MB/sec
   Mem-to-Mem DMA_SendCDB w/XOR xfer rate:       139 MB/sec
ADG SelfTestOK

PASSED: DMAXOR Controller Initialization

PASSED: Cache Controller Initialization

PAL_CO_Init: tbl_entries = 255 size = 142800
Start Up Complete
Memory start 47000000
Memory size 9000000
Cache Mem Test PASSED!


Pre-discovery LF: DIS: 0x00, SL_SAS: 0x00, SL_SATA: 0x00, LFV: 0x03, PBP: 0xff

Protocol device 0 scan devices started
Protocol device 0 scan devices done
Adapter 0 Bus Reset
PR 80aa10b8h:D000 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:02
PR 80aa10b8h:D001 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:02
PR 80aa10b8h:D002 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:02
PR 80aa10b8h:D250 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
get_drive_params: Inquiry to SEP for VPD page to get serial # failed.
Updated full box tbl in RIS

Configured logical unit (volume) count = 1
   ccf=0x00, mccf=0x00000000
Array A Unit 0: RAID 5; df=128 vs=OK drvs=3 dd=2 pg=1 vofs=0x000000000 blks=0x0222CE330 ca=ena srf=0x1 dt=2
  U0 drive map (hex) = 00 01 02
Controller WWID = 5001438007e874e0

*****  Discovered SAS (Compatible) Devices  ****
D000 p0|01 P1I[00-01]:Disk HP      DG0146FARVU     ,HPD8,WWID=5000cca0:0adf7b79, 10K
D001 p0|01 P1I[00-02]:Disk HP      DG0146FARVU     ,HPD8,WWID=5000cca0:0ae013c1, 10K
D002 p0|01 P1I[00-03]:Disk HP      DG0146FARVU     ,HPD8,WWID=5000cca0:0adc2171, 10K
D250 p0|01 ???[??-00]:SEP  PMCSIERA SRC 8x6G       ,RevC,WWID=50014380:07e874ef
D251 p0|01 ???[??-00]:SGPIO                        ,    ,WWID=50014380:07e874e0
D253                 :Protocol Adapter
D254                 :Protocol Adapter
Total Discovered SAS  Devices:  3

*****  Onboard PHY Link Rates  ****
   \PHYS         0          10         20         30         40
Onboard Phys   : AAA00000

*****  Expander PHY Link Rates  ****
EXP\PHYS         0          10         20         30         40
Total 6.0G Links:  3
DirtyQMemBytes: 147456
Local Memory Avail      7772092 bytes in 43 fragments
Shared Memory Avail     8367492 bytes in 17 fragments
Logical Reqs Avail      1023
Physical Reqs Avail     1022
Host Prefetch is ENABLED
ROM Flash Driver Init Passed
Testing ROM Image A
Testing ROM Image B
PCI rev. 0x1 using 4 lanes @5.0G

Host-to-local data xfer rate, using CPU:  588 MB/sec
Host-to-local data xfer rate, using DMA:  1399 MB/sec
Host time is 15:11:57, 5/14/2011
PCI slot 0
Periodic iLO command check interval=1 seconds, hostaddr=0x0DF63E020.
Host time is 15:11:59, 5/14/2011
PCI slot 0

[05/14 15:11:59]

Run-Time LF: DIS: 0x00, SL_SAS: 0x00, SL_SATA: 0x00, LFV: 0x03, PBP: 0xff

[05/14 15:12:02]Local-to-host data xfer rate, using DMA:  1454 MB/sec
[05/14 15:12:02]Int13 BIOS unit 0x80 = CISS LUN 0x4000000000000000 


Copyright (C) HP Corporation 1990-2010.
All rights reserved.
HP Array Controller Firmware Ver = 3.00, Build Num = 0
   BootBlock Ver = 2.07, HAL-PL Ver = 02.03.011.001
Compiled Feb 17 2010 14:42:36

PASSED: HAL API Initialization
FirstAvail : 0x80a1be40


Initializing Memory...

Physical Requests    1407
Logical Requests     1024
Command Lists        1025
Local Memory Avail      10735376 bytes in 5 fragments
Shared Memory Avail     8388600 bytes in 2 fragments
Logical Reqs Avail      1024
Physical Reqs Avail     1407
Host Prefetch is ENABLED
PASSED: Memory Initialization

SSID = 3245103c
PASSED: I2C Initialization

NVRAM Update: ILA returned 0x0
PASSED: Bootstrap NVRAM Checksum

Platform NVRAM auto-update found an embedded image, but it is not an upgrade

PASSED: Command I/O Initialization
PASSED: Timer Initialization

Board is Marble     Rev. C
Using WWID to generate new board serial #: 5001438007E874E
NumMgmtDevices = 105 MgmtDeviceStartIndex = 146
num_drive_params_entries = 255 drive params size = 49980

Diagnostic Pointers Initialized
Diagnostic download address = 0x817e8000
Initializing XOR Engine...
validate_pic_fw: pic version in ROM = 52
Battery 1 not present.
Battery 2 not present.
Battery 3 not present.

Battery Status:    Battery 1      Battery 2      Battery 3
---------------    ---------      ---------      ---------
Present:               NO             NO             NO
Responding:           N/A            N/A            N/A


Found 256 MB of cache memory.
wcxc_ram_start = 0x47000000
wcxc_ram_size  = 0x09000000
DIMM SN: PACCQ9SYWI29
Initializing ADG for SAS controllers only (tolerate 8 drive failure)
ADG keys initialized

Starting DMA SelfTest
   Pattern Fill DMA mem write xfer rate:         1673 MB/sec
   Pattern Fill DMA mem read xfer rate:          1872 MB/sec
   Zero Pattern Fill DMA mem write xfer rate:    1669 MB/sec
   Zero Pattern Fill DMA mem read xfer rate:     1872 MB/sec
   Mem-to-mem DMA xfer rate:                     906 MB/sec
   Mem-to-WXOR DMA xfer rate:                    623 MB/sec
   Mem-to-WXOR Multicast xfer rate:              800 MB/sec
   Mem-to-Mem DMA_SendCDB xfer rate:             163 MB/sec
   Mem-to-Mem DMA_SendCDB w/XOR xfer rate:       164 MB/sec
ADG SelfTestOK

PASSED: DMAXOR Controller Initialization

PASSED: Cache Controller Initialization

PAL_CO_Init: tbl_entries = 255 size = 142800
Start Up Complete
Memory start 47000000
Memory size 9000000
Cache Mem Test PASSED!


Pre-discovery LF: DIS: 0x00, SL_SAS: 0x00, SL_SATA: 0x00, LFV: 0x03, PBP: 0xff

Protocol device 0 scan devices started
Protocol device 0 scan devices done
Adapter 0 Bus Reset
PR 80aa10b8h:D000 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:02
PR 80aa10b8h:D001 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:02
PR 80aa10b8h:D002 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:02
PR 80aa10b8h:D250 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
get_drive_params: Inquiry to SEP for VPD page to get serial # failed.
Updated full box tbl in RIS

Configured logical unit (volume) count = 1
   ccf=0x00, mccf=0x00000000
Array A Unit 0: RAID 5; df=128 vs=OK drvs=3 dd=2 pg=1 vofs=0x000000000 blks=0x0222CE330 ca=ena srf=0x1 dt=2
  U0 drive map (hex) = 00 01 02
Controller WWID = 5001438007e874e0

*****  Discovered SAS (Compatible) Devices  ****
D000 p0|01 P1I[00-01]:Disk HP      DG0146FARVU     ,HPD8,WWID=5000cca0:0adf7b79, 10K
D001 p0|01 P1I[00-02]:Disk HP      DG0146FARVU     ,HPD8,WWID=5000cca0:0ae013c1, 10K
D002 p0|01 P1I[00-03]:Disk HP      DG0146FARVU     ,HPD8,WWID=5000cca0:0adc2171, 10K
D250 p0|01 ???[??-00]:SEP  PMCSIERA SRC 8x6G       ,RevC,WWID=50014380:07e874ef
D251 p0|01 ???[??-00]:SGPIO                        ,    ,WWID=50014380:07e874e0
D253                 :Protocol Adapter
D254                 :Protocol Adapter
Total Discovered SAS  Devices:  3

*****  Onboard PHY Link Rates  ****
   \PHYS         0          10         20         30         40
Onboard Phys   : AAA00000

*****  Expander PHY Link Rates  ****
EXP\PHYS         0          10         20         30         40
Total 6.0G Links:  3
DirtyQMemBytes: 147456
Local Memory Avail      7772092 bytes in 43 fragments
Shared Memory Avail     8367492 bytes in 17 fragments
Logical Reqs Avail      1023
Physical Reqs Avail     1022
Host Prefetch is ENABLED
ROM Flash Driver Init Passed
Testing ROM Image A
Testing ROM Image B
PCI rev. 0x1 using 4 lanes @5.0G

Host-to-local data xfer rate, using CPU:  593 MB/sec
Host-to-local data xfer rate, using DMA:  1382 MB/sec
Host time is 16:44:28, 5/14/2011
PCI slot 0
Periodic iLO command check interval=1 seconds, hostaddr=0x0DF63E020.
Host time is 16:44:29, 5/14/2011
PCI slot 0

[05/14 16:44:29]

Run-Time LF: DIS: 0x00, SL_SAS: 0x00, SL_SATA: 0x00, LFV: 0x03, PBP: 0xff

[05/14 16:44:32]Local-to-host data xfer rate, using DMA:  1464 MB/sec
[05/14 16:44:32]Int13 BIOS unit 0x80 = CISS LUN 0x4000000000000000 


Copyright (C) HP Corporation 1990-2010.
All rights reserved.
HP Array Controller Firmware Ver = 3.00, Build Num = 0
   BootBlock Ver = 2.07, HAL-PL Ver = 02.03.011.001
Compiled Feb 17 2010 14:42:36

PASSED: HAL API Initialization
FirstAvail : 0x80a1be40


Initializing Memory...

Physical Requests    1407
Logical Requests     1024
Command Lists        1025
Local Memory Avail      10735376 bytes in 5 fragments
Shared Memory Avail     8388600 bytes in 2 fragments
Logical Reqs Avail      1024
Physical Reqs Avail     1407
Host Prefetch is ENABLED
PASSED: Memory Initialization

SSID = 3245103c
PASSED: I2C Initialization

NVRAM Update: ILA returned 0x0
PASSED: Bootstrap NVRAM Checksum

Platform NVRAM auto-update found an embedded image, but it is not an upgrade

PASSED: Command I/O Initialization
PASSED: Timer Initialization

Board is Marble     Rev. C
Using WWID to generate new board serial #: 5001438007E874E
NumMgmtDevices = 105 MgmtDeviceStartIndex = 146
num_drive_params_entries = 255 drive params size = 49980

Diagnostic Pointers Initialized
Diagnostic download address = 0x817e8000
Initializing XOR Engine...
validate_pic_fw: pic version in ROM = 52
Battery 1 not present.
Battery 2 not present.
Battery 3 not present.

Battery Status:    Battery 1      Battery 2      Battery 3
---------------    ---------      ---------      ---------
Present:               NO             NO             NO
Responding:           N/A            N/A            N/A


Found 256 MB of cache memory.
wcxc_ram_start = 0x47000000
wcxc_ram_size  = 0x09000000
DIMM SN: PACCQ9SYWI29
Initializing ADG for SAS controllers only (tolerate 8 drive failure)
ADG keys initialized

Starting DMA SelfTest
   Pattern Fill DMA mem write xfer rate:         1671 MB/sec
   Pattern Fill DMA mem read xfer rate:          1873 MB/sec
   Zero Pattern Fill DMA mem write xfer rate:    1668 MB/sec
   Zero Pattern Fill DMA mem read xfer rate:     1873 MB/sec
   Mem-to-mem DMA xfer rate:                     914 MB/sec
   Mem-to-WXOR DMA xfer rate:                    617 MB/sec
   Mem-to-WXOR Multicast xfer rate:              790 MB/sec
   Mem-to-Mem DMA_SendCDB xfer rate:             168 MB/sec
   Mem-to-Mem DMA_SendCDB w/XOR xfer rate:       164 MB/sec
ADG SelfTestOK

PASSED: DMAXOR Controller Initialization

PASSED: Cache Controller Initialization

PAL_CO_Init: tbl_entries = 255 size = 142800
Start Up Complete
Memory start 47000000
Memory size 9000000
Cache Mem Test PASSED!


Pre-discovery LF: DIS: 0x00, SL_SAS: 0x00, SL_SATA: 0x00, LFV: 0x03, PBP: 0xff

Protocol device 0 scan devices started
Protocol device 0 scan devices done
Adapter 0 Bus Reset
PR 80aa10b8h:D000 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:02
PR 80aa10b8h:D001 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:02
PR 80aa10b8h:D002 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:02
PR 80aa10b8h:D250 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
get_drive_params: Inquiry to SEP for VPD page to get serial # failed.
Updated full box tbl in RIS

Configured logical unit (volume) count = 1
   ccf=0x00, mccf=0x00000000
Array A Unit 0: RAID 5; df=128 vs=OK drvs=3 dd=2 pg=1 vofs=0x000000000 blks=0x0222CE330 ca=ena srf=0x1 dt=2
  U0 drive map (hex) = 00 01 02
Controller WWID = 5001438007e874e0

*****  Discovered SAS (Compatible) Devices  ****
D000 p0|01 P1I[00-01]:Disk HP      DG0146FARVU     ,HPD8,WWID=5000cca0:0adf7b79, 10K
D001 p0|01 P1I[00-02]:Disk HP      DG0146FARVU     ,HPD8,WWID=5000cca0:0ae013c1, 10K
D002 p0|01 P1I[00-03]:Disk HP      DG0146FARVU     ,HPD8,WWID=5000cca0:0adc2171, 10K
D250 p0|01 ???[??-00]:SEP  PMCSIERA SRC 8x6G       ,RevC,WWID=50014380:07e874ef
D251 p0|01 ???[??-00]:SGPIO                        ,    ,WWID=50014380:07e874e0
D253                 :Protocol Adapter
D254                 :Protocol Adapter
Total Discovered SAS  Devices:  3

*****  Onboard PHY Link Rates  ****
   \PHYS         0          10         20         30         40
Onboard Phys   : AAA00000

*****  Expander PHY Link Rates  ****
EXP\PHYS         0          10         20         30         40
Total 6.0G Links:  3
DirtyQMemBytes: 147456
Local Memory Avail      7772092 bytes in 43 fragments
Shared Memory Avail     8367492 bytes in 17 fragments
Logical Reqs Avail      1023
Physical Reqs Avail     1020
Host Prefetch is ENABLED
ROM Flash Driver Init Passed
Testing ROM Image A
Testing ROM Image B
PCI rev. 0x1 using 4 lanes @5.0G

Host-to-local data xfer rate, using CPU:  583 MB/sec
Host-to-local data xfer rate, using DMA:  1384 MB/sec
Host time is 17:18:53, 5/14/2011
PCI slot 0
Periodic iLO command check interval=1 seconds, hostaddr=0x0DF63E020.
Host time is 17:18:55, 5/14/2011
PCI slot 0

[05/14 17:18:55]

Run-Time LF: DIS: 0x00, SL_SAS: 0x00, SL_SATA: 0x00, LFV: 0x03, PBP: 0xff

[05/14 17:18:58]Local-to-host data xfer rate, using DMA:  1462 MB/sec
[05/14 17:18:58]Int13 BIOS unit 0x80 = CISS LUN 0x4000000000000000 


Copyright (C) HP Corporation 1990-2010.
All rights reserved.
HP Array Controller Firmware Ver = 3.00, Build Num = 0
   BootBlock Ver = 2.07, HAL-PL Ver = 02.03.011.001
Compiled Feb 17 2010 14:42:36

PASSED: HAL API Initialization
FirstAvail : 0x80a1be40


Initializing Memory...

Physical Requests    1407
Logical Requests     1024
Command Lists        1025
Local Memory Avail      10735376 bytes in 5 fragments
Shared Memory Avail     8388600 bytes in 2 fragments
Logical Reqs Avail      1024
Physical Reqs Avail     1407
Host Prefetch is ENABLED
PASSED: Memory Initialization

SSID = 3245103c
PASSED: I2C Initialization

NVRAM Update: ILA returned 0x0
PASSED: Bootstrap NVRAM Checksum

Platform NVRAM auto-update found an embedded image, but it is not an upgrade

PASSED: Command I/O Initialization
PASSED: Timer Initialization

Board is Marble     Rev. C
Using WWID to generate new board serial #: 5001438007E874E
NumMgmtDevices = 105 MgmtDeviceStartIndex = 146
num_drive_params_entries = 255 drive params size = 49980

Diagnostic Pointers Initialized
Diagnostic download address = 0x817e8000
Initializing XOR Engine...
validate_pic_fw: pic version in ROM = 52
Battery 1 not present.
Battery 2 not present.
Battery 3 not present.

Battery Status:    Battery 1      Battery 2      Battery 3
---------------    ---------      ---------      ---------
Present:               NO             NO             NO
Responding:           N/A            N/A            N/A


Found 256 MB of cache memory.
wcxc_ram_start = 0x47000000
wcxc_ram_size  = 0x09000000
DIMM SN: PACCQ9SYWI29
Initializing ADG for SAS controllers only (tolerate 8 drive failure)
ADG keys initialized

Starting DMA SelfTest
   Pattern Fill DMA mem write xfer rate:         1668 MB/sec
   Pattern Fill DMA mem read xfer rate:          1873 MB/sec
   Zero Pattern Fill DMA mem write xfer rate:    1668 MB/sec
   Zero Pattern Fill DMA mem read xfer rate:     1873 MB/sec
   Mem-to-mem DMA xfer rate:                     905 MB/sec
   Mem-to-WXOR DMA xfer rate:                    616 MB/sec
   Mem-to-WXOR Multicast xfer rate:              792 MB/sec
   Mem-to-Mem DMA_SendCDB xfer rate:             156 MB/sec
   Mem-to-Mem DMA_SendCDB w/XOR xfer rate:       165 MB/sec
ADG SelfTestOK

PASSED: DMAXOR Controller Initialization

PASSED: Cache Controller Initialization

PAL_CO_Init: tbl_entries = 255 size = 142800
Start Up Complete
Memory start 47000000
Memory size 9000000
Cache Mem Test PASSED!


Pre-discovery LF: DIS: 0x00, SL_SAS: 0x00, SL_SATA: 0x00, LFV: 0x03, PBP: 0xff

Protocol device 0 scan devices started
Protocol device 0 scan devices done
Adapter 0 Bus Reset
PR 80aa10b8h:D000 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:02
PR 80aa10b8h:D001 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:02
PR 80aa10b8h:D002 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:02
PR 80aa10b8h:D250 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
get_drive_params: Inquiry to SEP for VPD page to get serial # failed.
Updated full box tbl in RIS

Configured logical unit (volume) count = 1
   ccf=0x00, mccf=0x00000000
Array A Unit 0: RAID 5; df=128 vs=OK drvs=3 dd=2 pg=1 vofs=0x000000000 blks=0x0222CE330 ca=ena srf=0x1 dt=2
  U0 drive map (hex) = 00 01 02
Controller WWID = 5001438007e874e0

*****  Discovered SAS (Compatible) Devices  ****
D000 p0|01 P1I[00-01]:Disk HP      DG0146FARVU     ,HPD8,WWID=5000cca0:0adf7b79, 10K
D001 p0|01 P1I[00-02]:Disk HP      DG0146FARVU     ,HPD8,WWID=5000cca0:0ae013c1, 10K
D002 p0|01 P1I[00-03]:Disk HP      DG0146FARVU     ,HPD8,WWID=5000cca0:0adc2171, 10K
D250 p0|01 ???[??-00]:SEP  PMCSIERA SRC 8x6G       ,RevC,WWID=50014380:07e874ef
D251 p0|01 ???[??-00]:SGPIO                        ,    ,WWID=50014380:07e874e0
D253                 :Protocol Adapter
D254                 :Protocol Adapter
Total Discovered SAS  Devices:  3

*****  Onboard PHY Link Rates  ****
   \PHYS         0          10         20         30         40
Onboard Phys   : AAA00000

*****  Expander PHY Link Rates  ****
EXP\PHYS         0          10         20         30         40
Total 6.0G Links:  3
DirtyQMemBytes: 147456
Local Memory Avail      7772092 bytes in 43 fragments
Shared Memory Avail     8367492 bytes in 17 fragments
Logical Reqs Avail      1023
Physical Reqs Avail     1020
Host Prefetch is ENABLED
ROM Flash Driver Init Passed
Testing ROM Image A
Testing ROM Image B
PCI rev. 0x1 using 4 lanes @5.0G

Host-to-local data xfer rate, using CPU:  636 MB/sec
Host-to-local data xfer rate, using DMA:  1399 MB/sec
Host time is 14:59:45, 5/17/2011
PCI slot 0
Periodic iLO command check interval=1 seconds, hostaddr=0x0DF63E020.
Host time is 14:59:46, 5/17/2011
PCI slot 0

[05/17 14:59:46]

Run-Time LF: DIS: 0x00, SL_SAS: 0x00, SL_SATA: 0x00, LFV: 0x03, PBP: 0xff

[05/17 14:59:49]Local-to-host data xfer rate, using DMA:  1381 MB/sec
[05/17 14:59:49]Int13 BIOS unit 0x80 = CISS LUN 0x4000000000000000 


Copyright (C) HP Corporation 1990-2010.
All rights reserved.
HP Array Controller Firmware Ver = 3.00, Build Num = 0
   BootBlock Ver = 2.07, HAL-PL Ver = 02.03.011.001
Compiled Feb 17 2010 14:42:36

PASSED: HAL API Initialization
FirstAvail : 0x80a1be40


Initializing Memory...

Physical Requests    1407
Logical Requests     1024
Command Lists        1025
Local Memory Avail      10735376 bytes in 5 fragments
Shared Memory Avail     8388600 bytes in 2 fragments
Logical Reqs Avail      1024
Physical Reqs Avail     1407
Host Prefetch is ENABLED
PASSED: Memory Initialization

SSID = 3245103c
PASSED: I2C Initialization

NVRAM Update: ILA returned 0x0
PASSED: Bootstrap NVRAM Checksum

Platform NVRAM auto-update found an embedded image, but it is not an upgrade

PASSED: Command I/O Initialization
PASSED: Timer Initialization

Board is Marble     Rev. C
Using WWID to generate new board serial #: 5001438007E874E
NumMgmtDevices = 105 MgmtDeviceStartIndex = 146
num_drive_params_entries = 255 drive params size = 49980

Diagnostic Pointers Initialized
Diagnostic download address = 0x817e8000
Initializing XOR Engine...
validate_pic_fw: pic version in ROM = 52
Battery 1 not present.
Battery 2 not present.
Battery 3 not present.

Battery Status:    Battery 1      Battery 2      Battery 3
---------------    ---------      ---------      ---------
Present:               NO             NO             NO
Responding:           N/A            N/A            N/A


Found 256 MB of cache memory.
wcxc_ram_start = 0x47000000
wcxc_ram_size  = 0x09000000
DIMM SN: PACCQ9SYWI29
Initializing ADG for SAS controllers only (tolerate 8 drive failure)
ADG keys initialized

Starting DMA SelfTest
   Pattern Fill DMA mem write xfer rate:         1672 MB/sec
   Pattern Fill DMA mem read xfer rate:          1872 MB/sec
   Zero Pattern Fill DMA mem write xfer rate:    1668 MB/sec
   Zero Pattern Fill DMA mem read xfer rate:     1873 MB/sec
   Mem-to-mem DMA xfer rate:                     897 MB/sec
   Mem-to-WXOR DMA xfer rate:                    620 MB/sec
   Mem-to-WXOR Multicast xfer rate:              811 MB/sec
   Mem-to-Mem DMA_SendCDB xfer rate:             151 MB/sec
   Mem-to-Mem DMA_SendCDB w/XOR xfer rate:       181 MB/sec
ADG SelfTestOK

PASSED: DMAXOR Controller Initialization

PASSED: Cache Controller Initialization

PAL_CO_Init: tbl_entries = 255 size = 142800
Start Up Complete
Memory start 47000000
Memory size 9000000
Cache Mem Test PASSED!


Pre-discovery LF: DIS: 0x00, SL_SAS: 0x00, SL_SATA: 0x00, LFV: 0x03, PBP: 0xff

Protocol device 0 scan devices started
Protocol device 0 scan devices done
Adapter 0 Bus Reset
PR 80aa10b8h:D000 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:02
PR 80aa10b8h:D001 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:02
PR 80aa10b8h:D002 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:02
PR 80aa10b8h:D250 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
get_drive_params: Inquiry to SEP for VPD page to get serial # failed.
Updated full box tbl in RIS

Configured logical unit (volume) count = 1
   ccf=0x00, mccf=0x00000000
Array A Unit 0: RAID 5; df=128 vs=OK drvs=3 dd=2 pg=1 vofs=0x000000000 blks=0x0222CE330 ca=ena srf=0x1 dt=2
  U0 drive map (hex) = 00 01 02
Controller WWID = 5001438007e874e0

*****  Discovered SAS (Compatible) Devices  ****
D000 p0|01 P1I[00-01]:Disk HP      DG0146FARVU     ,HPD8,WWID=5000cca0:0adf7b79, 10K
D001 p0|01 P1I[00-02]:Disk HP      DG0146FARVU     ,HPD8,WWID=5000cca0:0ae013c1, 10K
D002 p0|01 P1I[00-03]:Disk HP      DG0146FARVU     ,HPD8,WWID=5000cca0:0adc2171, 10K
D250 p0|01 ???[??-00]:SEP  PMCSIERA SRC 8x6G       ,RevC,WWID=50014380:07e874ef
D251 p0|01 ???[??-00]:SGPIO                        ,    ,WWID=50014380:07e874e0
D253                 :Protocol Adapter
D254                 :Protocol Adapter
Total Discovered SAS  Devices:  3

*****  Onboard PHY Link Rates  ****
   \PHYS         0          10         20         30         40
Onboard Phys   : AAA00000

*****  Expander PHY Link Rates  ****
EXP\PHYS         0          10         20         30         40
Total 6.0G Links:  3
DirtyQMemBytes: 147456
Local Memory Avail      7772092 bytes in 43 fragments
Shared Memory Avail     8367492 bytes in 17 fragments
Logical Reqs Avail      1024
Physical Reqs Avail     1024
Host Prefetch is ENABLED
ROM Flash Driver Init Passed
Testing ROM Image A
Testing ROM Image B
PCI rev. 0x1 using 4 lanes @5.0G

Host-to-local data xfer rate, using CPU:  656 MB/sec
Host-to-local data xfer rate, using DMA:  1398 MB/sec
Host time is 10:43:18, 5/23/2011
PCI slot 0
Periodic iLO command check interval=1 seconds, hostaddr=0x0DF63E020.
Host time is 10:43:20, 5/23/2011
PCI slot 0

[05/23 10:43:20]

Run-Time LF: DIS: 0x00, SL_SAS: 0x00, SL_SATA: 0x00, LFV: 0x03, PBP: 0xff

[05/23 10:43:23]Local-to-host data xfer rate, using DMA:  1459 MB/sec
[05/23 10:43:23]Int13 BIOS unit 0x80 = CISS LUN 0x4000000000000000 


Copyright (C) HP Corporation 1990-2010.
All rights reserved.
HP Array Controller Firmware Ver = 3.00, Build Num = 0
   BootBlock Ver = 2.07, HAL-PL Ver = 02.03.011.001
Compiled Feb 17 2010 14:42:36

PASSED: HAL API Initialization
FirstAvail : 0x80a1be40


Initializing Memory...

Physical Requests    1407
Logical Requests     1024
Command Lists        1025
Local Memory Avail      10735376 bytes in 5 fragments
Shared Memory Avail     8388600 bytes in 2 fragments
Logical Reqs Avail      1024
Physical Reqs Avail     1407
Host Prefetch is ENABLED
PASSED: Memory Initialization

SSID = 3245103c
PASSED: I2C Initialization

NVRAM Update: ILA returned 0x0
PASSED: Bootstrap NVRAM Checksum

Platform NVRAM auto-update found an embedded image, but it is not an upgrade

PASSED: Command I/O Initialization
PASSED: Timer Initialization

Board is Marble     Rev. C
Using WWID to generate new board serial #: 5001438007E874E
NumMgmtDevices = 105 MgmtDeviceStartIndex = 146
num_drive_params_entries = 255 drive params size = 49980

Diagnostic Pointers Initialized
Diagnostic download address = 0x817e8000
Initializing XOR Engine...
validate_pic_fw: pic version in ROM = 52
Battery 1 not present.
Battery 2 not present.
Battery 3 not present.

Battery Status:    Battery 1      Battery 2      Battery 3
---------------    ---------      ---------      ---------
Present:               NO             NO             NO
Responding:           N/A            N/A            N/A


Found 256 MB of cache memory.
wcxc_ram_start = 0x47000000
wcxc_ram_size  = 0x09000000
DIMM SN: PACCQ9SYWI29
Initializing ADG for SAS controllers only (tolerate 8 drive failure)
ADG keys initialized

Starting DMA SelfTest
   Pattern Fill DMA mem write xfer rate:         1669 MB/sec
   Pattern Fill DMA mem read xfer rate:          1874 MB/sec
   Zero Pattern Fill DMA mem write xfer rate:    1668 MB/sec
   Zero Pattern Fill DMA mem read xfer rate:     1874 MB/sec
   Mem-to-mem DMA xfer rate:                     904 MB/sec
   Mem-to-WXOR DMA xfer rate:                    614 MB/sec
   Mem-to-WXOR Multicast xfer rate:              793 MB/sec
   Mem-to-Mem DMA_SendCDB xfer rate:             161 MB/sec
   Mem-to-Mem DMA_SendCDB w/XOR xfer rate:       164 MB/sec
ADG SelfTestOK

PASSED: DMAXOR Controller Initialization

PASSED: Cache Controller Initialization

PAL_CO_Init: tbl_entries = 255 size = 142800
Start Up Complete
Memory start 47000000
Memory size 9000000
Cache Mem Test PASSED!


Pre-discovery LF: DIS: 0x00, SL_SAS: 0x00, SL_SATA: 0x00, LFV: 0x03, PBP: 0xff

Protocol device 0 scan devices started
Protocol device 0 scan devices done
Adapter 0 Bus Reset
PR 80aa10b8h:D000 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:02
PR 80aa10b8h:D001 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:02
PR 80aa10b8h:D002 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:02
PR 80aa10b8h:D250 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
get_drive_params: Inquiry to SEP for VPD page to get serial # failed.
Updated full box tbl in RIS

Configured logical unit (volume) count = 1
   ccf=0x00, mccf=0x00000000
Array A Unit 0: RAID 5; df=128 vs=OK drvs=3 dd=2 pg=1 vofs=0x000000000 blks=0x0222CE330 ca=ena srf=0x1 dt=2
  U0 drive map (hex) = 00 01 02
Controller WWID = 5001438007e874e0

*****  Discovered SAS (Compatible) Devices  ****
D000 p0|01 P1I[00-01]:Disk HP      DG0146FARVU     ,HPD8,WWID=5000cca0:0adf7b79, 10K
D001 p0|01 P1I[00-02]:Disk HP      DG0146FARVU     ,HPD8,WWID=5000cca0:0ae013c1, 10K
D002 p0|01 P1I[00-03]:Disk HP      DG0146FARVU     ,HPD8,WWID=5000cca0:0adc2171, 10K
D250 p0|01 ???[??-00]:SEP  PMCSIERA SRC 8x6G       ,RevC,WWID=50014380:07e874ef
D251 p0|01 ???[??-00]:SGPIO                        ,    ,WWID=50014380:07e874e0
D253                 :Protocol Adapter
D254                 :Protocol Adapter
Total Discovered SAS  Devices:  3

*****  Onboard PHY Link Rates  ****
   \PHYS         0          10         20         30         40
Onboard Phys   : AAA00000

*****  Expander PHY Link Rates  ****
EXP\PHYS         0          10         20         30         40
Total 6.0G Links:  3
DirtyQMemBytes: 147456
Local Memory Avail      7772092 bytes in 43 fragments
Shared Memory Avail     8367492 bytes in 17 fragments
Logical Reqs Avail      1023
Physical Reqs Avail     1020
Host Prefetch is ENABLED
ROM Flash Driver Init Passed
Testing ROM Image A
Testing ROM Image B
PCI rev. 0x1 using 4 lanes @5.0G

Host-to-local data xfer rate, using CPU:  654 MB/sec
Host-to-local data xfer rate, using DMA:  1402 MB/sec
Host time is 9:41:00, 8/16/2011
PCI slot 0
Periodic iLO command check interval=1 seconds, hostaddr=0x0DF63E020.
Host time is 9:41:02, 8/16/2011
PCI slot 0

[08/16 09:41:02]

Run-Time LF: DIS: 0x00, SL_SAS: 0x00, SL_SATA: 0x00, LFV: 0x03, PBP: 0xff

[08/16 09:41:05]Local-to-host data xfer rate, using DMA:  1464 MB/sec
[08/16 09:41:05]Int13 BIOS unit 0x80 = CISS LUN 0x4000000000000000 


Copyright (C) HP Corporation 1990-2010.
All rights reserved.
HP Array Controller Firmware Ver = 3.00, Build Num = 0
   BootBlock Ver = 2.07, HAL-PL Ver = 02.03.011.001
Compiled Feb 17 2010 14:42:36

PASSED: HAL API Initialization
FirstAvail : 0x80a1be40


Initializing Memory...

Physical Requests    1407
Logical Requests     1024
Command Lists        1025
Local Memory Avail      10735376 bytes in 5 fragments
Shared Memory Avail     8388600 bytes in 2 fragments
Logical Reqs Avail      1024
Physical Reqs Avail     1407
Host Prefetch is ENABLED
PASSED: Memory Initialization

SSID = 3245103c
PASSED: I2C Initialization

NVRAM Update: ILA returned 0x0
PASSED: Bootstrap NVRAM Checksum

Platform NVRAM auto-update found an embedded image, but it is not an upgrade

PASSED: Command I/O Initialization
PASSED: Timer Initialization

Board is Marble     Rev. C
Using WWID to generate new board serial #: 5001438007E874E
NumMgmtDevices = 105 MgmtDeviceStartIndex = 146
num_drive_params_entries = 255 drive params size = 49980

Diagnostic Pointers Initialized
Diagnostic download address = 0x817e8000
Initializing XOR Engine...
validate_pic_fw: pic version in ROM = 52
Battery 1 not present.
Battery 2 not present.
Battery 3 not present.

Battery Status:    Battery 1      Battery 2      Battery 3
---------------    ---------      ---------      ---------
Present:               NO             NO             NO
Responding:           N/A            N/A            N/A


Found 256 MB of cache memory.
wcxc_ram_start = 0x47000000
wcxc_ram_size  = 0x09000000
DIMM SN: PACCQ9SYWI29
Initializing ADG for SAS controllers only (tolerate 8 drive failure)
ADG keys initialized

Starting DMA SelfTest
   Pattern Fill DMA mem write xfer rate:         1672 MB/sec
   Pattern Fill DMA mem read xfer rate:          1873 MB/sec
   Zero Pattern Fill DMA mem write xfer rate:    1668 MB/sec
   Zero Pattern Fill DMA mem read xfer rate:     1873 MB/sec
   Mem-to-mem DMA xfer rate:                     909 MB/sec
   Mem-to-WXOR DMA xfer rate:                    617 MB/sec
   Mem-to-WXOR Multicast xfer rate:              792 MB/sec
   Mem-to-Mem DMA_SendCDB xfer rate:             153 MB/sec
   Mem-to-Mem DMA_SendCDB w/XOR xfer rate:       180 MB/sec
ADG SelfTestOK

PASSED: DMAXOR Controller Initialization

PASSED: Cache Controller Initialization

PAL_CO_Init: tbl_entries = 255 size = 142800
Start Up Complete
Memory start 47000000
Memory size 9000000
Cache Mem Test PASSED!


Pre-discovery LF: DIS: 0x00, SL_SAS: 0x00, SL_SATA: 0x00, LFV: 0x03, PBP: 0xff

Protocol device 0 scan devices started
Protocol device 0 scan devices done
Adapter 0 Bus Reset
PR 80aa10b8h:D000 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:02
PR 80aa10b8h:D001 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:02
PR 80aa10b8h:D002 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:02
PR 80aa10b8h:D250 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
get_drive_params: Inquiry to SEP for VPD page to get serial # failed.
Updated full box tbl in RIS

Configured logical unit (volume) count = 1
   ccf=0x00, mccf=0x00000000
Array A Unit 0: RAID 5; df=128 vs=OK drvs=3 dd=2 pg=1 vofs=0x000000000 blks=0x0222CE330 ca=ena srf=0x1 dt=2
  U0 drive map (hex) = 00 01 02
Controller WWID = 5001438007e874e0

*****  Discovered SAS (Compatible) Devices  ****
D000 p0|01 P1I[00-01]:Disk HP      DG0146FARVU     ,HPD8,WWID=5000cca0:0adf7b79, 10K
D001 p0|01 P1I[00-02]:Disk HP      DG0146FARVU     ,HPD8,WWID=5000cca0:0ae013c1, 10K
D002 p0|01 P1I[00-03]:Disk HP      DG0146FARVU     ,HPD8,WWID=5000cca0:0adc2171, 10K
D250 p0|01 ???[??-00]:SEP  PMCSIERA SRC 8x6G       ,RevC,WWID=50014380:07e874ef
D251 p0|01 ???[??-00]:SGPIO                        ,    ,WWID=50014380:07e874e0
D253                 :Protocol Adapter
D254                 :Protocol Adapter
Total Discovered SAS  Devices:  3

*****  Onboard PHY Link Rates  ****
   \PHYS         0          10         20         30         40
Onboard Phys   : AAA00000

*****  Expander PHY Link Rates  ****
EXP\PHYS         0          10         20         30         40
Total 6.0G Links:  3
DirtyQMemBytes: 147456
Local Memory Avail      7772092 bytes in 43 fragments
Shared Memory Avail     8367492 bytes in 17 fragments
Logical Reqs Avail      1024
Physical Reqs Avail     1024
Host Prefetch is ENABLED
ROM Flash Driver Init Passed
Testing ROM Image A
Testing ROM Image B
PCI rev. 0x1 using 4 lanes @5.0G

Host-to-local data xfer rate, using CPU:  658 MB/sec
Host-to-local data xfer rate, using DMA:  1399 MB/sec
Host time is 10:12:00, 8/16/2011
PCI slot 0
Periodic iLO command check interval=1 seconds, hostaddr=0x0DF63E020.
Host time is 10:12:02, 8/16/2011
PCI slot 0

[08/16 10:12:02]

Run-Time LF: DIS: 0x00, SL_SAS: 0x00, SL_SATA: 0x00, LFV: 0x03, PBP: 0xff

[08/16 10:12:05]Local-to-host data xfer rate, using DMA:  1460 MB/sec
[08/16 10:12:05]Int13 BIOS unit 0x80 = CISS LUN 0x4000000000000000 


Copyright (C) HP Corporation 1990-2010.
All rights reserved.
HP Array Controller Firmware Ver = 3.00, Build Num = 0
   BootBlock Ver = 2.07, HAL-PL Ver = 02.03.011.001
Compiled Feb 17 2010 14:42:36

PASSED: HAL API Initialization
FirstAvail : 0x80a1be40


Initializing Memory...

Physical Requests    1407
Logical Requests     1024
Command Lists        1025
Local Memory Avail      10735376 bytes in 5 fragments
Shared Memory Avail     8388600 bytes in 2 fragments
Logical Reqs Avail      1024
Physical Reqs Avail     1407
Host Prefetch is ENABLED
PASSED: Memory Initialization

SSID = 3245103c
PASSED: I2C Initialization

NVRAM Update: ILA returned 0x0
PASSED: Bootstrap NVRAM Checksum

Platform NVRAM auto-update found an embedded image, but it is not an upgrade

PASSED: Command I/O Initialization
PASSED: Timer Initialization

Board is Marble     Rev. C
Using WWID to generate new board serial #: 5001438007E874E
NumMgmtDevices = 105 MgmtDeviceStartIndex = 146
num_drive_params_entries = 255 drive params size = 49980

Diagnostic Pointers Initialized
Diagnostic download address = 0x817e8000
Initializing XOR Engine...
validate_pic_fw: pic version in ROM = 52
Battery 1 not present.
Battery 2 not present.
Battery 3 not present.

Battery Status:    Battery 1      Battery 2      Battery 3
---------------    ---------      ---------      ---------
Present:               NO             NO             NO
Responding:           N/A            N/A            N/A


Found 256 MB of cache memory.
wcxc_ram_start = 0x47000000
wcxc_ram_size  = 0x09000000
DIMM SN: PACCQ9SYWI29
Initializing ADG for SAS controllers only (tolerate 8 drive failure)
ADG keys initialized

Starting DMA SelfTest
   Pattern Fill DMA mem write xfer rate:         1669 MB/sec
   Pattern Fill DMA mem read xfer rate:          1874 MB/sec
   Zero Pattern Fill DMA mem write xfer rate:    1668 MB/sec
   Zero Pattern Fill DMA mem read xfer rate:     1874 MB/sec
   Mem-to-mem DMA xfer rate:                     905 MB/sec
   Mem-to-WXOR DMA xfer rate:                    615 MB/sec
   Mem-to-WXOR Multicast xfer rate:              782 MB/sec
   Mem-to-Mem DMA_SendCDB xfer rate:             168 MB/sec
   Mem-to-Mem DMA_SendCDB w/XOR xfer rate:       179 MB/sec
ADG SelfTestOK

PASSED: DMAXOR Controller Initialization

PASSED: Cache Controller Initialization

PAL_CO_Init: tbl_entries = 255 size = 142800
Start Up Complete
Memory start 47000000
Memory size 9000000
Cache Mem Test PASSED!


Pre-discovery LF: DIS: 0x00, SL_SAS: 0x00, SL_SATA: 0x00, LFV: 0x03, PBP: 0xff

Protocol device 0 scan devices started
Protocol device 0 scan devices done
Adapter 0 Bus Reset
PR 80aa10b8h:D000 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:02
PR 80aa10b8h:D001 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:02
PR 80aa10b8h:D002 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:02
PR 80aa10b8h:D250 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
get_drive_params: Inquiry to SEP for VPD page to get serial # failed.
Updated full box tbl in RIS

Configured logical unit (volume) count = 1
   ccf=0x00, mccf=0x00000000
Array A Unit 0: RAID 5; df=128 vs=OK drvs=3 dd=2 pg=1 vofs=0x000000000 blks=0x0222CE330 ca=ena srf=0x1 dt=2
  U0 drive map (hex) = 00 01 02
Controller WWID = 5001438007e874e0

*****  Discovered SAS (Compatible) Devices  ****
D000 p0|01 P1I[00-01]:Disk HP      DG0146FARVU     ,HPD8,WWID=5000cca0:0adf7b79, 10K
D001 p0|01 P1I[00-02]:Disk HP      DG0146FARVU     ,HPD8,WWID=5000cca0:0ae013c1, 10K
D002 p0|01 P1I[00-03]:Disk HP      DG0146FARVU     ,HPD8,WWID=5000cca0:0adc2171, 10K
D250 p0|01 ???[??-00]:SEP  PMCSIERA SRC 8x6G       ,RevC,WWID=50014380:07e874ef
D251 p0|01 ???[??-00]:SGPIO                        ,    ,WWID=50014380:07e874e0
D253                 :Protocol Adapter
D254                 :Protocol Adapter
Total Discovered SAS  Devices:  3

*****  Onboard PHY Link Rates  ****
   \PHYS         0          10         20         30         40
Onboard Phys   : AAA00000

*****  Expander PHY Link Rates  ****
EXP\PHYS         0          10         20         30         40
Total 6.0G Links:  3
DirtyQMemBytes: 147456
Local Memory Avail      7772092 bytes in 43 fragments
Shared Memory Avail     8367492 bytes in 17 fragments
Logical Reqs Avail      1023
Physical Reqs Avail     1020
Host Prefetch is ENABLED
ROM Flash Driver Init Passed
Testing ROM Image A
Testing ROM Image B
PCI rev. 0x1 using 4 lanes @5.0G

Host-to-local data xfer rate, using CPU:  650 MB/sec
Host-to-local data xfer rate, using DMA:  1401 MB/sec
Host time is 10:43:04, 8/16/2011
PCI slot 0
Periodic iLO command check interval=1 seconds, hostaddr=0x0DF63E020.
Host time is 10:43:06, 8/16/2011
PCI slot 0

[08/16 10:43:06]

Run-Time LF: DIS: 0x00, SL_SAS: 0x00, SL_SATA: 0x00, LFV: 0x03, PBP: 0xff

[08/16 10:43:09]Local-to-host data xfer rate, using DMA:  1460 MB/sec
[08/16 10:43:09]Int13 BIOS unit 0x80 = CISS LUN 0x4000000000000000 


Copyright (C) HP Corporation 1990-2010.
All rights reserved.
HP Array Controller Firmware Ver = 3.00, Build Num = 0
   BootBlock Ver = 2.07, HAL-PL Ver = 02.03.011.001
Compiled Feb 17 2010 14:42:36

PASSED: HAL API Initialization
FirstAvail : 0x80a1be40


Initializing Memory...

Physical Requests    1407
Logical Requests     1024
Command Lists        1025
Local Memory Avail      10735376 bytes in 5 fragments
Shared Memory Avail     8388600 bytes in 2 fragments
Logical Reqs Avail      1024
Physical Reqs Avail     1407
Host Prefetch is ENABLED
PASSED: Memory Initialization

SSID = 3245103c
PASSED: I2C Initialization

NVRAM Update: ILA returned 0x0
PASSED: Bootstrap NVRAM Checksum

Platform NVRAM auto-update found an embedded image, but it is not an upgrade

PASSED: Command I/O Initialization
PASSED: Timer Initialization

Board is Marble     Rev. C
Using WWID to generate new board serial #: 5001438007E874E
NumMgmtDevices = 105 MgmtDeviceStartIndex = 146
num_drive_params_entries = 255 drive params size = 49980

Diagnostic Pointers Initialized
Diagnostic download address = 0x817e8000
Initializing XOR Engine...
validate_pic_fw: pic version in ROM = 52
Battery 1 not present.
Battery 2 not present.
Battery 3 not present.

Battery Status:    Battery 1      Battery 2      Battery 3
---------------    ---------      ---------      ---------
Present:               NO             NO             NO
Responding:           N/A            N/A            N/A


Found 256 MB of cache memory.
wcxc_ram_start = 0x47000000
wcxc_ram_size  = 0x09000000
DIMM SN: PACCQ9SYWI29
Initializing ADG for SAS controllers only (tolerate 8 drive failure)
ADG keys initialized

Starting DMA SelfTest
   Pattern Fill DMA mem write xfer rate:         1671 MB/sec
   Pattern Fill DMA mem read xfer rate:          1873 MB/sec
   Zero Pattern Fill DMA mem write xfer rate:    1668 MB/sec
   Zero Pattern Fill DMA mem read xfer rate:     1873 MB/sec
   Mem-to-mem DMA xfer rate:                     913 MB/sec
   Mem-to-WXOR DMA xfer rate:                    614 MB/sec
   Mem-to-WXOR Multicast xfer rate:              814 MB/sec
   Mem-to-Mem DMA_SendCDB xfer rate:             153 MB/sec
   Mem-to-Mem DMA_SendCDB w/XOR xfer rate:       179 MB/sec
ADG SelfTestOK

PASSED: DMAXOR Controller Initialization

PASSED: Cache Controller Initialization

PAL_CO_Init: tbl_entries = 255 size = 142800
Start Up Complete
Memory start 47000000
Memory size 9000000
Cache Mem Test PASSED!


Pre-discovery LF: DIS: 0x00, SL_SAS: 0x00, SL_SATA: 0x00, LFV: 0x03, PBP: 0xff

Protocol device 0 scan devices started
Protocol device 0 scan devices done
Adapter 0 Bus Reset
PR 80aa10b8h:D000 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:02
PR 80aa10b8h:D001 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:02
PR 80aa10b8h:D002 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:02
PR 80aa10b8h:D250 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
get_drive_params: Inquiry to SEP for VPD page to get serial # failed.
Updated full box tbl in RIS

Configured logical unit (volume) count = 1
   ccf=0x00, mccf=0x00000000
Array A Unit 0: RAID 5; df=128 vs=OK drvs=3 dd=2 pg=1 vofs=0x000000000 blks=0x0222CE330 ca=ena srf=0x1 dt=2
  U0 drive map (hex) = 00 01 02
Controller WWID = 5001438007e874e0

*****  Discovered SAS (Compatible) Devices  ****
D000 p0|01 P1I[00-01]:Disk HP      DG0146FARVU     ,HPD8,WWID=5000cca0:0adf7b79, 10K
D001 p0|01 P1I[00-02]:Disk HP      DG0146FARVU     ,HPD8,WWID=5000cca0:0ae013c1, 10K
D002 p0|01 P1I[00-03]:Disk HP      DG0146FARVU     ,HPD8,WWID=5000cca0:0adc2171, 10K
D250 p0|01 ???[??-00]:SEP  PMCSIERA SRC 8x6G       ,RevC,WWID=50014380:07e874ef
D251 p0|01 ???[??-00]:SGPIO                        ,    ,WWID=50014380:07e874e0
D253                 :Protocol Adapter
D254                 :Protocol Adapter
Total Discovered SAS  Devices:  3

*****  Onboard PHY Link Rates  ****
   \PHYS         0          10         20         30         40
Onboard Phys   : AAA00000

*****  Expander PHY Link Rates  ****
EXP\PHYS         0          10         20         30         40
Total 6.0G Links:  3
DirtyQMemBytes: 147456
Local Memory Avail      7772092 bytes in 43 fragments
Shared Memory Avail     8367492 bytes in 17 fragments
Logical Reqs Avail      1023
Physical Reqs Avail     1020
Host Prefetch is ENABLED
ROM Flash Driver Init Passed
Testing ROM Image A
Testing ROM Image B
PCI rev. 0x1 using 4 lanes @5.0G

Host-to-local data xfer rate, using CPU:  653 MB/sec
Host-to-local data xfer rate, using DMA:  1382 MB/sec
Host time is 10:15:10, 10/24/2011
PCI slot 0
Periodic iLO command check interval=1 seconds, hostaddr=0x0DF63E020.
Host time is 10:15:11, 10/24/2011
PCI slot 0

[10/24 10:15:11]

Run-Time LF: DIS: 0x00, SL_SAS: 0x00, SL_SATA: 0x00, LFV: 0x03, PBP: 0xff

[10/24 10:15:14]Local-to-host data xfer rate, using DMA:  1439 MB/sec
[10/24 10:15:14]Int13 BIOS unit 0x80 = CISS LUN 0x4000000000000000 


Copyright (C) HP Corporation 1990-2010.
All rights reserved.
HP Array Controller Firmware Ver = 3.00, Build Num = 0
   BootBlock Ver = 2.07, HAL-PL Ver = 02.03.011.001
Compiled Feb 17 2010 14:42:36

PASSED: HAL API Initialization
FirstAvail : 0x80a1be40


Initializing Memory...

Physical Requests    1407
Logical Requests     1024
Command Lists        1025
Local Memory Avail      10735376 bytes in 5 fragments
Shared Memory Avail     8388600 bytes in 2 fragments
Logical Reqs Avail      1024
Physical Reqs Avail     1407
Host Prefetch is ENABLED
PASSED: Memory Initialization

SSID = 3245103c
PASSED: I2C Initialization

NVRAM Update: ILA returned 0x0
PASSED: Bootstrap NVRAM Checksum

Platform NVRAM auto-update found an embedded image, but it is not an upgrade

PASSED: Command I/O Initialization
PASSED: Timer Initialization

Board is Marble     Rev. C
Using WWID to generate new board serial #: 5001438007E874E
NumMgmtDevices = 105 MgmtDeviceStartIndex = 146
num_drive_params_entries = 255 drive params size = 49980

Diagnostic Pointers Initialized
Diagnostic download address = 0x817e8000
Initializing XOR Engine...
validate_pic_fw: pic version in ROM = 52
Battery 1 not present.
Battery 2 not present.
Battery 3 not present.

Battery Status:    Battery 1      Battery 2      Battery 3
---------------    ---------      ---------      ---------
Present:               NO             NO             NO
Responding:           N/A            N/A            N/A


Found 256 MB of cache memory.
wcxc_ram_start = 0x47000000
wcxc_ram_size  = 0x09000000
DIMM SN: PACCQ9SYWI29
Initializing ADG for SAS controllers only (tolerate 8 drive failure)
ADG keys initialized

Starting DMA SelfTest
   Pattern Fill DMA mem write xfer rate:         1669 MB/sec
   Pattern Fill DMA mem read xfer rate:          1873 MB/sec
   Zero Pattern Fill DMA mem write xfer rate:    1667 MB/sec
   Zero Pattern Fill DMA mem read xfer rate:     1875 MB/sec
   Mem-to-mem DMA xfer rate:                     912 MB/sec
   Mem-to-WXOR DMA xfer rate:                    626 MB/sec
   Mem-to-WXOR Multicast xfer rate:              792 MB/sec
   Mem-to-Mem DMA_SendCDB xfer rate:             167 MB/sec
   Mem-to-Mem DMA_SendCDB w/XOR xfer rate:       170 MB/sec
ADG SelfTestOK

PASSED: DMAXOR Controller Initialization

PASSED: Cache Controller Initialization

PAL_CO_Init: tbl_entries = 255 size = 142800
Start Up Complete
Memory start 47000000
Memory size 9000000
Cache Mem Test PASSED!


Pre-discovery LF: DIS: 0x00, SL_SAS: 0x00, SL_SATA: 0x00, LFV: 0x03, PBP: 0xff

Protocol device 0 scan devices started
Protocol device 0 scan devices done
Adapter 0 Bus Reset
PR 80aa10b8h:D000 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:02
PR 80aa10b8h:D001 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:02
PR 80aa10b8h:D002 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:02
PR 80aa10b8h:D250 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
get_drive_params: Inquiry to SEP for VPD page to get serial # failed.
Updated full box tbl in RIS

Configured logical unit (volume) count = 1
   ccf=0x00, mccf=0x00000000
Array A Unit 0: RAID 5; df=128 vs=OK drvs=3 dd=2 pg=1 vofs=0x000000000 blks=0x0222CE330 ca=ena srf=0x1 dt=2
  U0 drive map (hex) = 00 01 02
Controller WWID = 5001438007e874e0

*****  Discovered SAS (Compatible) Devices  ****
D000 p0|01 P1I[00-01]:Disk HP      DG0146FARVU     ,HPD8,WWID=5000cca0:0adf7b79, 10K
D001 p0|01 P1I[00-02]:Disk HP      DG0146FARVU     ,HPD8,WWID=5000cca0:0ae013c1, 10K
D002 p0|01 P1I[00-03]:Disk HP      DG0146FARVU     ,HPD8,WWID=5000cca0:0adc2171, 10K
D250 p0|01 ???[??-00]:SEP  PMCSIERA SRC 8x6G       ,RevC,WWID=50014380:07e874ef
D251 p0|01 ???[??-00]:SGPIO                        ,    ,WWID=50014380:07e874e0
D253                 :Protocol Adapter
D254                 :Protocol Adapter
Total Discovered SAS  Devices:  3

*****  Onboard PHY Link Rates  ****
   \PHYS         0          10         20         30         40
Onboard Phys   : AAA00000

*****  Expander PHY Link Rates  ****
EXP\PHYS         0          10         20         30         40
Total 6.0G Links:  3
DirtyQMemBytes: 147456
Local Memory Avail      7772092 bytes in 43 fragments
Shared Memory Avail     8367492 bytes in 17 fragments
Logical Reqs Avail      1023
Physical Reqs Avail     1020
Host Prefetch is ENABLED
ROM Flash Driver Init Passed
Testing ROM Image A
Testing ROM Image B
PCI rev. 0x1 using 4 lanes @5.0G

Host-to-local data xfer rate, using CPU:  586 MB/sec
Host-to-local data xfer rate, using DMA:  1387 MB/sec
Host time is 16:37:26, 10/24/2011
PCI slot 0
Periodic iLO command check interval=1 seconds, hostaddr=0x0DF63E020.
Host time is 16:37:28, 10/24/2011
PCI slot 0

[10/24 16:37:28]

Run-Time LF: DIS: 0x00, SL_SAS: 0x00, SL_SATA: 0x00, LFV: 0x03, PBP: 0xff

[10/24 16:37:31]Local-to-host data xfer rate, using DMA:  1423 MB/sec
[10/24 16:37:31]Int13 BIOS unit 0x80 = CISS LUN 0x4000000000000000 


Copyright (C) HP Corporation 1990-2010.
All rights reserved.
HP Array Controller Firmware Ver = 3.00, Build Num = 0
   BootBlock Ver = 2.07, HAL-PL Ver = 02.03.011.001
Compiled Feb 17 2010 14:42:36

PASSED: HAL API Initialization
FirstAvail : 0x80a1be40


Initializing Memory...

Physical Requests    1407
Logical Requests     1024
Command Lists        1025
Local Memory Avail      10735376 bytes in 5 fragments
Shared Memory Avail     8388600 bytes in 2 fragments
Logical Reqs Avail      1024
Physical Reqs Avail     1407
Host Prefetch is ENABLED
PASSED: Memory Initialization

SSID = 3245103c
PASSED: I2C Initialization

NVRAM Update: ILA returned 0x0
PASSED: Bootstrap NVRAM Checksum

Platform NVRAM auto-update found an embedded image, but it is not an upgrade

PASSED: Command I/O Initialization
PASSED: Timer Initialization

Board is Marble     Rev. C
Using WWID to generate new board serial #: 5001438007E874E
NumMgmtDevices = 105 MgmtDeviceStartIndex = 146
num_drive_params_entries = 255 drive params size = 49980

Diagnostic Pointers Initialized
Diagnostic download address = 0x817e8000
Initializing XOR Engine...
validate_pic_fw: pic version in ROM = 52
Battery 1 not present.
Battery 2 not present.
Battery 3 not present.

Battery Status:    Battery 1      Battery 2      Battery 3
---------------    ---------      ---------      ---------
Present:               NO             NO             NO
Responding:           N/A            N/A            N/A


Found 256 MB of cache memory.
wcxc_ram_start = 0x47000000
wcxc_ram_size  = 0x09000000
DIMM SN: PACCQ9SYWI29
Initializing ADG for SAS controllers only (tolerate 8 drive failure)
ADG keys initialized

Starting DMA SelfTest
   Pattern Fill DMA mem write xfer rate:         1671 MB/sec
   Pattern Fill DMA mem read xfer rate:          1873 MB/sec
   Zero Pattern Fill DMA mem write xfer rate:    1668 MB/sec
   Zero Pattern Fill DMA mem read xfer rate:     1873 MB/sec
   Mem-to-mem DMA xfer rate:                     906 MB/sec
   Mem-to-WXOR DMA xfer rate:                    618 MB/sec
   Mem-to-WXOR Multicast xfer rate:              783 MB/sec
   Mem-to-Mem DMA_SendCDB xfer rate:             158 MB/sec
   Mem-to-Mem DMA_SendCDB w/XOR xfer rate:       180 MB/sec
ADG SelfTestOK

PASSED: DMAXOR Controller Initialization

PASSED: Cache Controller Initialization

PAL_CO_Init: tbl_entries = 255 size = 142800
Start Up Complete
Memory start 47000000
Memory size 9000000
Cache Mem Test PASSED!


Pre-discovery LF: DIS: 0x00, SL_SAS: 0x00, SL_SATA: 0x00, LFV: 0x03, PBP: 0xff

Protocol device 0 scan devices started
Protocol device 0 scan devices done
Adapter 0 Bus Reset
PR 80aa10b8h:D000 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:02
PR 80aa10b8h:D001 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:02
PR 80aa10b8h:D002 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:02
PR 80aa10b8h:D250 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
get_drive_params: Inquiry to SEP for VPD page to get serial # failed.
Updated full box tbl in RIS

Configured logical unit (volume) count = 1
   ccf=0x00, mccf=0x00000000
Array A Unit 0: RAID 5; df=128 vs=OK drvs=3 dd=2 pg=1 vofs=0x000000000 blks=0x0222CE330 ca=ena srf=0x1 dt=2
  U0 drive map (hex) = 00 01 02
Controller WWID = 5001438007e874e0

*****  Discovered SAS (Compatible) Devices  ****
D000 p0|01 P1I[00-01]:Disk HP      DG0146FARVU     ,HPD8,WWID=5000cca0:0adf7b79, 10K
D001 p0|01 P1I[00-02]:Disk HP      DG0146FARVU     ,HPD8,WWID=5000cca0:0ae013c1, 10K
D002 p0|01 P1I[00-03]:Disk HP      DG0146FARVU     ,HPD8,WWID=5000cca0:0adc2171, 10K
D250 p0|01 ???[??-00]:SEP  PMCSIERA SRC 8x6G       ,RevC,WWID=50014380:07e874ef
D251 p0|01 ???[??-00]:SGPIO                        ,    ,WWID=50014380:07e874e0
D253                 :Protocol Adapter
D254                 :Protocol Adapter
Total Discovered SAS  Devices:  3

*****  Onboard PHY Link Rates  ****
   \PHYS         0          10         20         30         40
Onboard Phys   : AAA00000

*****  Expander PHY Link Rates  ****
EXP\PHYS         0          10         20         30         40
Total 6.0G Links:  3
DirtyQMemBytes: 147456
Local Memory Avail      7772092 bytes in 43 fragments
Shared Memory Avail     8367492 bytes in 17 fragments
Logical Reqs Avail      1023
Physical Reqs Avail     1020
Host Prefetch is ENABLED
ROM Flash Driver Init Passed
Testing ROM Image A
Testing ROM Image B
PCI rev. 0x1 using 4 lanes @5.0G

Host-to-local data xfer rate, using CPU:  654 MB/sec
Host-to-local data xfer rate, using DMA:  1402 MB/sec
Host time is 18:41:30, 10/24/2011
PCI slot 0
Periodic iLO command check interval=1 seconds, hostaddr=0x0DF63E020.
Host time is 18:41:32, 10/24/2011
PCI slot 0

[10/24 18:41:32]

Run-Time LF: DIS: 0x00, SL_SAS: 0x00, SL_SATA: 0x00, LFV: 0x03, PBP: 0xff

[10/24 18:41:35]Local-to-host data xfer rate, using DMA:  1465 MB/sec
[10/24 18:41:35]Int13 BIOS unit 0x80 = CISS LUN 0x4000000000000000 


Copyright (C) HP Corporation 1990-2010.
All rights reserved.
HP Array Controller Firmware Ver = 3.00, Build Num = 0
   BootBlock Ver = 2.07, HAL-PL Ver = 02.03.011.001
Compiled Feb 17 2010 14:42:36

PASSED: HAL API Initialization
FirstAvail : 0x80a1be40


Initializing Memory...

Physical Requests    1407
Logical Requests     1024
Command Lists        1025
Local Memory Avail      10735376 bytes in 5 fragments
Shared Memory Avail     8388600 bytes in 2 fragments
Logical Reqs Avail      1024
Physical Reqs Avail     1407
Host Prefetch is ENABLED
PASSED: Memory Initialization

SSID = 3245103c
PASSED: I2C Initialization

NVRAM Update: ILA returned 0x0
PASSED: Bootstrap NVRAM Checksum

Platform NVRAM auto-update found an embedded image, but it is not an upgrade

PASSED: Command I/O Initialization
PASSED: Timer Initialization

Board is Marble     Rev. C
Using WWID to generate new board serial #: 5001438007E874E
NumMgmtDevices = 105 MgmtDeviceStartIndex = 146
num_drive_params_entries = 255 drive params size = 49980

Diagnostic Pointers Initialized
Diagnostic download address = 0x817e8000
Initializing XOR Engine...
validate_pic_fw: pic version in ROM = 52
Battery 1 not present.
Battery 2 not present.
Battery 3 not present.

Battery Status:    Battery 1      Battery 2      Battery 3
---------------    ---------      ---------      ---------
Present:               NO             NO             NO
Responding:           N/A            N/A            N/A


Found 256 MB of cache memory.
wcxc_ram_start = 0x47000000
wcxc_ram_size  = 0x09000000
DIMM SN: PACCQ9SYWI29
Initializing ADG for SAS controllers only (tolerate 8 drive failure)
ADG keys initialized

Starting DMA SelfTest
   Pattern Fill DMA mem write xfer rate:         1672 MB/sec
   Pattern Fill DMA mem read xfer rate:          1873 MB/sec
   Zero Pattern Fill DMA mem write xfer rate:    1669 MB/sec
   Zero Pattern Fill DMA mem read xfer rate:     1874 MB/sec
   Mem-to-mem DMA xfer rate:                     908 MB/sec
   Mem-to-WXOR DMA xfer rate:                    617 MB/sec
   Mem-to-WXOR Multicast xfer rate:              793 MB/sec
   Mem-to-Mem DMA_SendCDB xfer rate:             165 MB/sec
   Mem-to-Mem DMA_SendCDB w/XOR xfer rate:       165 MB/sec
ADG SelfTestOK

PASSED: DMAXOR Controller Initialization

PASSED: Cache Controller Initialization

PAL_CO_Init: tbl_entries = 255 size = 142800
Start Up Complete
Memory start 47000000
Memory size 9000000
Cache Mem Test PASSED!


Pre-discovery LF: DIS: 0x00, SL_SAS: 0x00, SL_SATA: 0x00, LFV: 0x03, PBP: 0xff

Protocol device 0 scan devices started
Protocol device 0 scan devices done
Adapter 0 Bus Reset
PR 80aa10b8h:D000 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:02
PR 80aa10b8h:D001 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:02
PR 80aa10b8h:D002 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:02
PR 80aa10b8h:D250 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
get_drive_params: Inquiry to SEP for VPD page to get serial # failed.
Updated full box tbl in RIS

Configured logical unit (volume) count = 1
   ccf=0x00, mccf=0x00000000
Array A Unit 0: RAID 5; df=128 vs=OK drvs=3 dd=2 pg=1 vofs=0x000000000 blks=0x0222CE330 ca=ena srf=0x1 dt=2
  U0 drive map (hex) = 00 01 02
Controller WWID = 5001438007e874e0

*****  Discovered SAS (Compatible) Devices  ****
D000 p0|01 P1I[00-01]:Disk HP      DG0146FARVU     ,HPD8,WWID=5000cca0:0adf7b79, 10K
D001 p0|01 P1I[00-02]:Disk HP      DG0146FARVU     ,HPD8,WWID=5000cca0:0ae013c1, 10K
D002 p0|01 P1I[00-03]:Disk HP      DG0146FARVU     ,HPD8,WWID=5000cca0:0adc2171, 10K
D250 p0|01 ???[??-00]:SEP  PMCSIERA SRC 8x6G       ,RevC,WWID=50014380:07e874ef
D251 p0|01 ???[??-00]:SGPIO                        ,    ,WWID=50014380:07e874e0
D253                 :Protocol Adapter
D254                 :Protocol Adapter
Total Discovered SAS  Devices:  3

*****  Onboard PHY Link Rates  ****
   \PHYS         0          10         20         30         40
Onboard Phys   : AAA00000

*****  Expander PHY Link Rates  ****
EXP\PHYS         0          10         20         30         40
Total 6.0G Links:  3
DirtyQMemBytes: 147456
Local Memory Avail      7772092 bytes in 43 fragments
Shared Memory Avail     8367492 bytes in 17 fragments
Logical Reqs Avail      1023
Physical Reqs Avail     1020
Host Prefetch is ENABLED
ROM Flash Driver Init Passed
Testing ROM Image A
Testing ROM Image B
PCI rev. 0x1 using 4 lanes @5.0G

Host-to-local data xfer rate, using CPU:  633 MB/sec
Host-to-local data xfer rate, using DMA:  1398 MB/sec
Host time is 7:38:57, 11/19/2011
PCI slot 0
Periodic iLO command check interval=1 seconds, hostaddr=0x0DF63E020.
Host time is 7:38:59, 11/19/2011
PCI slot 0

[11/19 07:38:59]

Run-Time LF: DIS: 0x00, SL_SAS: 0x00, SL_SATA: 0x00, LFV: 0x03, PBP: 0xff

[11/19 07:39:02]Local-to-host data xfer rate, using DMA:  1464 MB/sec
[11/19 07:39:02]Int13 BIOS unit 0x80 = CISS LUN 0x4000000000000000 


Copyright (C) HP Corporation 1990-2010.
All rights reserved.
HP Array Controller Firmware Ver = 3.00, Build Num = 0
   BootBlock Ver = 2.07, HAL-PL Ver = 02.03.011.001
Compiled Feb 17 2010 14:42:36

PASSED: HAL API Initialization
FirstAvail : 0x80a1be40


Initializing Memory...

Physical Requests    1407
Logical Requests     1024
Command Lists        1025
Local Memory Avail      10735376 bytes in 5 fragments
Shared Memory Avail     8388600 bytes in 2 fragments
Logical Reqs Avail      1024
Physical Reqs Avail     1407
Host Prefetch is ENABLED
PASSED: Memory Initialization

SSID = 3245103c
PASSED: I2C Initialization

NVRAM Update: ILA returned 0x0
PASSED: Bootstrap NVRAM Checksum

Platform NVRAM auto-update found an embedded image, but it is not an upgrade

PASSED: Command I/O Initialization
PASSED: Timer Initialization

Board is Marble     Rev. C
Using WWID to generate new board serial #: 5001438007E874E
NumMgmtDevices = 105 MgmtDeviceStartIndex = 146
num_drive_params_entries = 255 drive params size = 49980

Diagnostic Pointers Initialized
Diagnostic download address = 0x817e8000
Initializing XOR Engine...
validate_pic_fw: pic version in ROM = 52
Battery 1 not present.
Battery 2 not present.
Battery 3 not present.

Battery Status:    Battery 1      Battery 2      Battery 3
---------------    ---------      ---------      ---------
Present:               NO             NO             NO
Responding:           N/A            N/A            N/A


Found 256 MB of cache memory.
wcxc_ram_start = 0x47000000
wcxc_ram_size  = 0x09000000
DIMM SN: PACCQ9SYWI29
Initializing ADG for SAS controllers only (tolerate 8 drive failure)
ADG keys initialized

Starting DMA SelfTest
   Pattern Fill DMA mem write xfer rate:         1673 MB/sec
   Pattern Fill DMA mem read xfer rate:          1872 MB/sec
   Zero Pattern Fill DMA mem write xfer rate:    1670 MB/sec
   Zero Pattern Fill DMA mem read xfer rate:     1872 MB/sec
   Mem-to-mem DMA xfer rate:                     909 MB/sec
   Mem-to-WXOR DMA xfer rate:                    616 MB/sec
   Mem-to-WXOR Multicast xfer rate:              802 MB/sec
   Mem-to-Mem DMA_SendCDB xfer rate:             155 MB/sec
   Mem-to-Mem DMA_SendCDB w/XOR xfer rate:       180 MB/sec
ADG SelfTestOK

PASSED: DMAXOR Controller Initialization

PASSED: Cache Controller Initialization

PAL_CO_Init: tbl_entries = 255 size = 142800
Start Up Complete
Memory start 47000000
Memory size 9000000
Cache Mem Test PASSED!


Pre-discovery LF: DIS: 0x00, SL_SAS: 0x00, SL_SATA: 0x00, LFV: 0x03, PBP: 0xff

Protocol device 0 scan devices started
Protocol device 0 scan devices done
Adapter 0 Bus Reset
PR 80aa10b8h:D000 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:02
PR 80aa10b8h:D001 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:02
PR 80aa10b8h:D002 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:02
PR 80aa10b8h:D250 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
get_drive_params: Inquiry to SEP for VPD page to get serial # failed.
Updated full box tbl in RIS

Configured logical unit (volume) count = 1
   ccf=0x00, mccf=0x00000000
Array A Unit 0: RAID 5; df=128 vs=OK drvs=3 dd=2 pg=1 vofs=0x000000000 blks=0x0222CE330 ca=ena srf=0x1 dt=2
  U0 drive map (hex) = 00 01 02
Controller WWID = 5001438007e874e0

*****  Discovered SAS (Compatible) Devices  ****
D000 p0|01 P1I[00-01]:Disk HP      DG0146FARVU     ,HPD8,WWID=5000cca0:0adf7b79, 10K
D001 p0|01 P1I[00-02]:Disk HP      DG0146FARVU     ,HPD8,WWID=5000cca0:0ae013c1, 10K
D002 p0|01 P1I[00-03]:Disk HP      DG0146FARVU     ,HPD8,WWID=5000cca0:0adc2171, 10K
D250 p0|01 ???[??-00]:SEP  PMCSIERA SRC 8x6G       ,RevC,WWID=50014380:07e874ef
D251 p0|01 ???[??-00]:SGPIO                        ,    ,WWID=50014380:07e874e0
D253                 :Protocol Adapter
D254                 :Protocol Adapter
Total Discovered SAS  Devices:  3

*****  Onboard PHY Link Rates  ****
   \PHYS         0          10         20         30         40
Onboard Phys   : AAA00000

*****  Expander PHY Link Rates  ****
EXP\PHYS         0          10         20         30         40
Total 6.0G Links:  3
DirtyQMemBytes: 147456
Local Memory Avail      7772092 bytes in 43 fragments
Shared Memory Avail     8367492 bytes in 17 fragments
Logical Reqs Avail      1023
Physical Reqs Avail     1020
Host Prefetch is ENABLED
ROM Flash Driver Init Passed
Testing ROM Image A
Testing ROM Image B
PCI rev. 0x1 using 4 lanes @5.0G

Host-to-local data xfer rate, using CPU:  590 MB/sec
Host-to-local data xfer rate, using DMA:  1373 MB/sec
Host time is 1:52:36, 12/15/2011
PCI slot 0
Periodic iLO command check interval=1 seconds, hostaddr=0x0DF63E020.
Host time is 1:52:38, 12/15/2011
PCI slot 0

[12/15 01:52:38]

Run-Time LF: DIS: 0x00, SL_SAS: 0x00, SL_SATA: 0x00, LFV: 0x03, PBP: 0xff

[12/15 01:52:41]Local-to-host data xfer rate, using DMA:  1464 MB/sec
[12/15 01:52:41]Int13 BIOS unit 0x80 = CISS LUN 0x4000000000000000 


Copyright (C) HP Corporation 1990-2010.
All rights reserved.
HP Array Controller Firmware Ver = 3.00, Build Num = 0
   BootBlock Ver = 2.07, HAL-PL Ver = 02.03.011.001
Compiled Feb 17 2010 14:42:36

PASSED: HAL API Initialization
FirstAvail : 0x80a1be40


Initializing Memory...

Physical Requests    1407
Logical Requests     1024
Command Lists        1025
Local Memory Avail      10735376 bytes in 5 fragments
Shared Memory Avail     8388600 bytes in 2 fragments
Logical Reqs Avail      1024
Physical Reqs Avail     1407
Host Prefetch is ENABLED
PASSED: Memory Initialization

SSID = 3245103c
PASSED: I2C Initialization

NVRAM Update: ILA returned 0x0
PASSED: Bootstrap NVRAM Checksum

Platform NVRAM auto-update found an embedded image, but it is not an upgrade

PASSED: Command I/O Initialization
PASSED: Timer Initialization

Board is Marble     Rev. C
Using WWID to generate new board serial #: 5001438007E874E
NumMgmtDevices = 105 MgmtDeviceStartIndex = 146
num_drive_params_entries = 255 drive params size = 49980

Diagnostic Pointers Initialized
Diagnostic download address = 0x817e8000
Initializing XOR Engine...
validate_pic_fw: pic version in ROM = 52
Battery 1 not present.
Battery 2 not present.
Battery 3 not present.

Battery Status:    Battery 1      Battery 2      Battery 3
---------------    ---------      ---------      ---------
Present:               NO             NO             NO
Responding:           N/A            N/A            N/A


Found 256 MB of cache memory.
wcxc_ram_start = 0x47000000
wcxc_ram_size  = 0x09000000
DIMM SN: PACCQ9SYWI29
Initializing ADG for SAS controllers only (tolerate 8 drive failure)
ADG keys initialized

Starting DMA SelfTest
   Pattern Fill DMA mem write xfer rate:         1672 MB/sec
   Pattern Fill DMA mem read xfer rate:          1874 MB/sec
   Zero Pattern Fill DMA mem write xfer rate:    1667 MB/sec
   Zero Pattern Fill DMA mem read xfer rate:     1872 MB/sec
   Mem-to-mem DMA xfer rate:                     911 MB/sec
   Mem-to-WXOR DMA xfer rate:                    619 MB/sec
   Mem-to-WXOR Multicast xfer rate:              788 MB/sec
   Mem-to-Mem DMA_SendCDB xfer rate:             155 MB/sec
   Mem-to-Mem DMA_SendCDB w/XOR xfer rate:       178 MB/sec
ADG SelfTestOK

PASSED: DMAXOR Controller Initialization

PASSED: Cache Controller Initialization

PAL_CO_Init: tbl_entries = 255 size = 142800
Start Up Complete
Memory start 47000000
Memory size 9000000
Cache Mem Test PASSED!


Pre-discovery LF: DIS: 0x00, SL_SAS: 0x00, SL_SATA: 0x00, LFV: 0x03, PBP: 0xff

Protocol device 0 scan devices started
Protocol device 0 scan devices done
Adapter 0 Bus Reset
PR 80aa10b8h:D000 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:02
PR 80aa10b8h:D001 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:02
PR 80aa10b8h:D002 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:02
PR 80aa10b8h:D250 Op=00 PLErr=02 IopErr=04 S=02 KCQ=6:29:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
PR 80aa10b8h:D250 Op=12 PLErr=02 IopErr=04 S=02 KCQ=5:24:00
get_drive_params: Inquiry to SEP for VPD page to get serial # failed.
Updated full box tbl in RIS

Configured logical unit (volume) count = 1
   ccf=0x00, mccf=0x00000000
Array A Unit 0: RAID 5; df=128 vs=OK drvs=3 dd=2 pg=1 vofs=0x000000000 blks=0x0222CE330 ca=ena srf=0x1 dt=2
  U0 drive map (hex) = 00 01 02
Controller WWID = 5001438007e874e0

*****  Discovered SAS (Compatible) Devices  ****
D000 p0|01 P1I[00-01]:Disk HP      DG0146FARVU     ,HPD8,WWID=5000cca0:0adf7b79, 10K
D001 p0|01 P1I[00-02]:Disk HP      DG0146FARVU     ,HPD8,WWID=5000cca0:0ae013c1, 10K
D002 p0|01 P1I[00-03]:Disk HP      DG0146FARVU     ,HPD8,WWID=5000cca0:0adc2171, 10K
D250 p0|01 ???[??-00]:SEP  PMCSIERA SRC 8x6G       ,RevC,WWID=50014380:07e874ef
D251 p0|01 ???[??-00]:SGPIO                        ,    ,WWID=50014380:07e874e0
D253                 :Protocol Adapter
D254                 :Protocol Adapter
Total Discovered SAS  Devices:  3

*****  Onboard PHY Link Rates  ****
   \PHYS         0          10         20         30         40
Onboard Phys   : AAA00000

*****  Expander PHY Link Rates  ****
EXP\PHYS         0          10         20         30         40
Total 6.0G Links:  3
DirtyQMemBytes: 147456
Local Memory Avail      7772092 bytes in 43 fragments
Shared Memory Avail     8367492 bytes in 17 fragments
Logical Reqs Avail      1023
Physical Reqs Avail     1022
Host Prefetch is ENABLED
ROM Flash Driver Init Passed
Testing ROM Image A
Testing ROM Image B
PCI rev. 0x1 using 4 lanes @5.0G

Host-to-local data xfer rate, using CPU:  624 MB/sec
Host-to-local data xfer rate, using DMA:  1396 MB/sec
Host time is 3:43:52, 3/09/2012
PCI slot 0
Periodic iLO command check interval=1 seconds, hostaddr=0x0DF63E020.
Host time is 3:43:54, 3/09/2012
PCI slot 0

[03/09 03:43:54]

Run-Time LF: DIS: 0x00, SL_SAS: 0x00, SL_SATA: 0x00, LFV: 0x03, PBP: 0xff

[03/09 03:43:57]Local-to-host data xfer rate, using DMA:  1369 MB/sec
[03/09 03:43:57]Int13 BIOS unit 0x80 = CISS LUN 0x4000000000000000 
[03/09 14:35:44]ACCESSING device 1: I2C address=a0:0 size=1024 at Offset 0
[03/09 14:35:44]READ SUCCESS: 1024 bytes of I2C device 1
