-------------------------------------------------    
HP Array Configuration Utility                    	 
------------------------------------------------- 	 

   ACU CLI Version: 8.40-4.0
   SoulAPI Version: 5.2.29.0

-------------------------------------------------   
Array Controllers  				 
------------------------------------------------- 	 

Smart Array P410i in Slot 0 (Embedded)    (sn: 5001438007E874E0)

------------------------------------------------- 	 
Controller Status                                 	 
------------------------------------------------- 	 

Smart Array P410i in Slot 0 (Embedded)
   Controller Status: OK
   Cache Status: OK


                                                  
------------------------------------------------- 
Smart Array P410i in Slot 0 				       
------------------------------------------------- 

Smart Array P410i in Slot 0 (Embedded)

   Array: A
      Interface Type: SAS
      Unused Space: 0 MB
      Status: OK




Smart Array P410i in Slot 0 (Embedded)    (sn: 5001438007E874E0)

   array A (SAS, Unused Space: 0 MB)


      logicaldrive 1 (273.4 GB, RAID 5, OK)

      physicaldrive 1I:1:1 (port 1I:box 1:bay 1, SAS, 146 GB, OK)
      physicaldrive 1I:1:2 (port 1I:box 1:bay 2, SAS, 146 GB, OK)
      physicaldrive 1I:1:3 (port 1I:box 1:bay 3, SAS, 146 GB, OK)

   sep 250 (WWID: 5001438007E874EF)

                                                  
                                                  
                                                  
------------------------------------------------- 
Smart Array P410i in Slot 0 - Detailed Configuration	       
------------------------------------------------- 

Smart Array P410i in Slot 0 (Embedded)
   Bus Interface: PCI
   Slot: 0
   Serial Number: 5001438007E874E0
   Cache Serial Number: PACCQ9SYWI29
   RAID 6 (ADG) Status: Disabled
   Controller Status: OK
   Chassis Slot: 
   Hardware Revision: Rev C
   Firmware Version: 3.00
   Rebuild Priority: Medium
   Expand Priority: Medium
   Surface Scan Delay: 15 secs
   Queue Depth: Automatic
   Monitor and Performance Delay: 60 min
   Elevator Sort: Enabled
   Degraded Performance Optimization: Disabled
   Inconsistency Repair Policy: Disabled
   Wait for Cache Room: Disabled
   Surface Analysis Inconsistency Notification: Disabled
   Post Prompt Timeout: 0 secs
   Cache Board Present: True
   Cache Status: OK
   Accelerator Ratio: 100% Read / 0% Write
   Drive Write Cache: Disabled
   Total Cache Size: 256 MB
   No-Battery Write Cache: Disabled
   Battery/Capacitor Count: 0
   SATA NCQ Supported: True

   Array: A
      Interface Type: SAS
      Unused Space: 0 MB
      Status: OK



      Logical Drive: 1
         Size: 273.4 GB
         Fault Tolerance: RAID 5
         Heads: 255
         Sectors Per Track: 32
         Cylinders: 65535
         Stripe Size: 64 KB
         Status: OK
         Array Accelerator: Enabled
         Parity Initialization Status: Initialization Completed
         Unique Identifier: 600508B1001030374538373445300300
         Disk Name: \\.\PhysicalDrive0
         Mount Points: C:\ 52.0 GB, D:\ 97.7 GB, E:\ 123.7 GB
         Logical Drive Label: A017149C5001438007E874E0F4E5

      physicaldrive 1I:1:1
         Port: 1I
         Box: 1
         Bay: 1
         Status: OK
         Drive Type: Data Drive
         Interface Type: SAS
         Size: 146 GB
         Rotational Speed: 10000
         Firmware Revision: HPD8
         Serial Number:         PCYYX40E
         Model: HP      DG0146FARVU     
         PHY Count: 2
         PHY Transfer Rate: 6.0GBPS, Unknown
      physicaldrive 1I:1:2
         Port: 1I
         Box: 1
         Bay: 2
         Status: OK
         Drive Type: Data Drive
         Interface Type: SAS
         Size: 146 GB
         Rotational Speed: 10000
         Firmware Revision: HPD8
         Serial Number:         PCYZ78DE
         Model: HP      DG0146FARVU     
         PHY Count: 2
         PHY Transfer Rate: 6.0GBPS, Unknown
      physicaldrive 1I:1:3
         Port: 1I
         Box: 1
         Bay: 3
         Status: OK
         Drive Type: Data Drive
         Interface Type: SAS
         Size: 146 GB
         Rotational Speed: 10000
         Firmware Revision: HPD8
         Serial Number:         PCYX1ZLE
         Model: HP      DG0146FARVU     
         PHY Count: 2
         PHY Transfer Rate: 6.0GBPS, Unknown

   sep 250
      Device Number: 250
      Firmware Version: RevC
      WWID: 5001438007E874EF
      Vendor ID: PMCSIERA
      Product ID:  SRC 8x6G       

